;
; OS/2 NIF Network Information File
; for the sk98nd.os2 v7.00 NDIS driver supporting the
; Marvell Yukon 88E8056 Adapter PCI-E Chipset
;
; (C)Copyright 2004 Marvell(R).
; All rights reserved.
;

[SK98ND]
 Type = NDIS
 Title = "Marvell Yukon 88E8056 PCI-E Adapter (APIC)"
 Version = 7.00
 Drivername= SK98ND$
 Xports = NETBEUI LANDD

[File]
 Name = M88E8056.OS2
 Path = IBMCOM\MACS

[BusNum]
Display = "PCI bus number"
Type = Decimal
Range = 0 - 255
Optional = Yes
Editable = Yes
Virtual = No
Help = "This parameter lets you specify the PCI bus number in which the
 Marvell Yukon 88E8056 Adapter resides.
 This parameter is not specified by default, which lets the driver
 automatically find the next unused device. You will usually not want to
 specify this parameter unless you have more than one
 Marvell Yukon 88E8056 Adapter installed
 in your system and you want to specify which particular device shall be
 used. Note that you must also specify the PCI device number parameter
 when you specify the PCI bus number parameter."

[DevNum]
Display = "PCI device number"
Type = Decimal
Range = 0 - 31
Optional = Yes
Editable = Yes
Virtual = No
Help = "This parameter lets you specify the PCI device number on the PCI
 bus in which the
 Marvell Yukon 88E8056 Adapter resides.
 This parameter is not specified by default, which lets the driver
 automatically find the next unused device. You will usually not want to
 specify this parameter unless you have more than one
 Marvell Yukon 88E8056 Adapter installed
 in your system and you want to specify which particular device shall be
 used. Note that you must also specify the PCI bus number parameter when
 you specify the PCI device number parameter."

[NetAddress]
Display = "Network adapter address"
Type = HexString
StrLength = 12
Optional = Yes
Editable = Yes
Virtual = No
Help = "This parameter overrides the network address of the
 Marvell Yukon 88E8056 Adapter.
 The value of this parameter is a string of 12 hexadecimal digits. The
 address must be unique among all other network adapter addresses on the
 network. Note that the second digit of the network address must be an
 even number (i.e. 0, 2, ... C, E)."

[MaxReceives]
Display = "Number of receive buffers"
Type = Decimal
Default = 30
Range = 3 - 40
Optional = Yes
Editable = Yes
Virtual = No
Help = "This parameter specifies the number of receive buffers The network
 adapter driver allocates approximately 1.5 kilobytes for each receive
 buffer. The value of this parameter should be high enough to accommodate
 the sum of all Number of Receive Buffers parameter values for all
 protocol drivers using the
 Marvell Yukon 88E8056 Adapter concurrently."

[MaxTransmits]
Display = "Maximum number of queued transmits"
Type = Decimal
Default = 30
Range = 1 - 50
Optional = Yes
Editable = Yes
Virtual = No
Help = "This parameter specifies the maximum number of transmit queue
 entries. The network adapter driver allocates approximately 80 bytes for
 each transmit queue entry. The value of this parameter should be high
 enough to accommodate the sum of all Maximum Number of Queued Transmits
 parameter values for all protocol drivers using the
 Marvell Yukon 88E8056 Adapter concurrently."

[ConType]
Display = "Connection type"
Type = String
StrLength = 5
Default = AUTO
Set = AUTO, 100FD, 100HD, 10FD, 10HD
Optional = Yes
Editable = Yes
Virtual = No
Help = "This parameter can be used to force link speed (10/100 Mbps) and
 duplex mode (full=FD vs. half=HD). Available values are AUTO, 100FD,
 100HD, 10FD, 10HD. Using other values than AUTO turns off
 auto-negotiation and is not recommended."
