[NVETH]
 Type       = NDIS
 Title      = "NVIDIA MAC Driver from Mensys BV"
 Version    = 0.1.6
 DriverName = NVETH$
 XPORTS     = NETBEUI, LANDD

[File]
 Name     = NVETH.OS2
 Path     = \IBMCOM\MACS

[MODE]
Display    = "Medium Type"
Type       = String
StrLength  = 10
Set        = "10HALF", "10FULL", "100HALF", "100FULL", "1000HALF", "1000FULL"
Optional   = Yes
Editable   = Yes
Help       = "This parameter specifies the link speed and connection type.
If not specified, it defaults to autodetection."

[OPTIMIZE]
Display    = "Use throughput optimization"
Type       = String
Strlength  = 4
Default    = "YES"
Set        = "YES", "NO"
Optional   = yes
Editable   = yes
Help       = "This parameter specifies whatever driver must fullfill throughput
optimization. If not specified, it defaults to YES."

[TIMER]
Display    = "Use HW timer"
Type       = String
Strlength  = 4
Default    = "NO"
Set        = "YES", "NO"
Optional   = yes
Editable   = yes
Help       = "This parameter specifies whatever driver must activate NVIDIA
hardware IRQ timer. If not specified, it defaults to NO."

[LINK_TIMER]
Display    = "Use link timer"
Type       = String
Strlength  = 4
Default    = "NO"
Set        = "YES", "NO"
Optional   = yes
Editable   = yes
Help       = "This parameter specifies whatever driver must periodically test
link. If not specified, it defaults to NO."

[RXCHAIN]
Display    = "Use receive chain instead of receive lookahead"
Type       = String
Strlength  = 4
Default    = "YES"
Set        = "YES", "NO"
Optional   = yes
Editable   = yes
Help       = "Use receive chain instead of receive lookahead. If not specified,
it defaults to YES."

[NETADDRESS]
Display    = "Network Adapter Address"
Type       = hexstring
Strlength  = 12
Optional   = yes
Editable   = yes
Help       = "This parameter overrides the network address of the network
 adapter card.	The value of this parameter is a hexadecimal string of
 12 digits.  The address must be unique among all other network adapter addresses on the network."
