[MCS7830]
   Type = NDIS_MULT
   Title = "Moschip USB2.0 to Ethernet Adapter"
   Version = 1.00
   Drivername = MCS7830$
   Xports = NETBEUI LANDD

[FILE]
   Name = MCS7830.OS2

[ETHERMODE]
   display = "Set Ethernet Speed and Duplex Mode"
   type = Decimal
   set = 0, 1, 2, 3, 4
   default = 0
   optional = YES
   editable = YES
   help = "The driver can configure the adapter for either Half or Full Duplex and
 10 Mbps or 100 Mbps. Values are: 0 (Autodetect)  1 (10Mbps/Half)  2 (10Mbps/Full)
  3 (100Mbps/Half)  4 (100Mbps/Full). Please note,
 Automatic detection of Full Duplex REQUIRES a hub with ports which are capable
 of performing N-Way auto-negotiation, so forcing the duplex mode to Full is
 recommended for most users connecting to a Full Duplex hub."

[NODE]
   display = "Locally Administered Address"
   type = String
   strlength = 12
   optional = YES
   editable = YES
   help = "Use this parameter to modify the network address used by
 the adapter."

[SERIALNR]
   display = "Serial Number Identifier"
   type = String
   strlength = 12
   optional = YES
   editable = YES
   help = "Use this parameter to allow connection to only the one
 adapter with selected Serial Number (readout via Hardware-Manager)."

