; IBM Token Ring Card

;* hlp.cardid = Card ID got from Version/Product Information
;* val.port1 = 0xA20
;* hlp.port1 = I/O Port Base Address 1
;* val.port2 = 0
;* hlp.port2 = I/O Port Base Address 2 (Not required)
;* val.irq = 3,4,5,6,7,9,10,11,12,13,14,15
;* hlp.irq = Interrupt (IRQ) Level
;* val.window1 = 0xC0000,0xC2000,0xC4000,0xC6000,0xC8000,0xCA000,0xCC000
;* val.window1 = 0xCE000,0xD0000,0xD2000,0xD4000,0xD6000,0xD8000,0xDA000
;* val.window1 = 0xDC000,0xDE000
;* hlp.window1 = Memory Mapped I/O (MMIO) Address
;* val.size1 = 0x2000
;* hlp.size1 = Size of Memory Mapped I/O (MMIO) Area (8KB)
;* val.offset1 = 0xC0000,0xC2000,0xC4000,0xC6000,0xC8000,0xCA000,0xCC000
;* val.offset1 = 0xCE000,0xD0000,0xD2000,0xD4000,0xD6000,0xD8000,0xDA000
;* val.offset1 = 0xDC000,0xDE000
;* hlp.offset1 = Card Offset for Memory Mapped I/O (MMIO) Area. It must be
;* hlp.offset1 = the same as Memory Mapped I/O (MMIO) address.
;* val.window2 = 0xC0000,0xC4000,0xC8000,0xCC000,0xD0000,0xD4000,0xD8000,0xDC000
;* hlp.window2 = Shared RAM (SRAM) Address
;* val.size2 = 0x2000,0x4000,0x8000,0x10000
;* hlp.size2 = Size of Shared RAM (SRAM)
;* val.offset2 = 0xC0000,0xC4000,0xC8000,0xCC000,0xD0000,0xD4000,0xD8000,0xDC000
;* hlp.offset2 = Card Offset for Shared RAM (SRAM). It must be the same as
;* hlp.offset2 = Shared RAM (SRAM) address.

CardID         =TOKEN RING
FunctionID     =0xFF
ManufacturerID =0xFFFF
IgnoreCardID   =
EnableSequence =ReqIO(0xA20,0xFF,0,0,0,0,0xFF)
                ReqIRQ(0,9)
                ReqConfig(0xFF,0xFF,0xFF,0x20,0,0,0x40)
                ReqWindow(1,0x000C,0xCA000,0x2000,0xFF)
                MapMemPage(1,0xCA000)
                ReqWindow(2,0x000C,0xCC000,0x4000,0xFF)
                MapMemPage(2,0xCC000)
                IBM_TokenRing(4)
                End
DisableSequence=End
