
  PC Card Director installation Programs

    Optional Parameters :

      PCMINST2 /S:<product source> /R:<specific response file>
               /R:<group response file> /L1:<error log file>
               /L2:<history log file> /T:<target>

      - If the "/S:<..>" is not specified, the installation programs
        assume that CID is not required, and work as normal mode which
        need user intervention.


          /S:   Specify the drive and path to the PCD files existing
                on the SDM code server.

                Exp. of valid /S: parameter :

                  /S:d:     /S:d:\      /S:d:\ppp       /S:d:\ppp\

                  d:   drive name (A-Z,a-z)
                  ppp: path name


          /T:   Specify the target drive and path for the product
                installation at the client workstation.

                Exp. of valid /T: parameter :

                  /T:d:     /T:d:\      /T:d:\ppp       /T:d:\ppp\

                  d:   drive name (A-Z,a-z)
                  ppp: path name


          /R:   Specify the drive, path and name to the client response
                file existing on the SDM code server.

                Exp. of valid /R: parameter :

                  /R:           (assumes PCMINST2.RSP in the source path)
                  /R:fff        (assumes fff in the source path)
                  /R:d:\ppp\fff

                  d:   drive name (A-Z,a-z)
                  ppp: path name
                  fff: response file name


          /G:   Specify the drive, path and name to the group response
                file existing on the SDM code server.

                Exp. of valid /G: parameter :

                  /G:           (assumes PCMINST2.RSP in the source path)
                  /G:fff        (assumes fff in the source path)
                  /G:d:\ppp\fff

                  d:   drive name (A-Z,a-z)
                  ppp: path name
                  fff: response file name


          /L1:  Specify the drive, path and name to the error log file
                existing on the SDM code server.

                Exp. of valid /L1: parameter :

                  /L1:           (assumes PCMINST2.ERR in the source path)
                  /L1:fff        (assumes fff in the source path)
                  /L1:d:\ppp\fff

                  d:   drive name (A-Z,a-z)
                  ppp: path name
                  fff: response file name


          /L2:  Specify the drive, path and name to the error history file
                existing on the SDM code server.

                Exp. of valid /L2: parameter :

                  /L2:           (assumes PCMINST2.HST in the source path)
                  /L2:fff        (assumes fff in the source path)
                  /L2:d:\ppp\fff

                  d:   drive name (A-Z,a-z)
                  ppp: path name
                  fff: response file name



    Response File Format :

      +-------------------------------------+
      |                                     |
      | #--- Comment -------------          |
      | Target=C:\TEST                      |
      | ReBoot=N                            |
      | UpdateConfig=Y                      |
      | ForceReplace=Y                      |
      | Use2ndSS=N                          |
      | *--- Comment -------------          |
      |                                     |
      +-------------------------------------+

        Target=
                Specify the target drive and path for the product
                installation at the client workstation.

                Exp. of valid Target= keyword :

                  Target=d:   TARGET=d:\    TaRgEt=d:\ppp   Target=d:\ppp\

                  d:   drive name (A-Z,a-z)
                  ppp: path name

        ReBoot=
                This keyword is valid only for OS/2. If the PCD for OS/2
                is installed to the system which has already been installed
                previous PCD, current installation program removes the
                previous PCD and then asks user to re-boot the system.
                Under the latest Warp, this re-booting is not necessary,
                but old one need this. This keyword specify the re-boot the
                client workstation or not, if the workstation has old PCD.
                The default setting is No.

                Exp. of valid ReBoot= keyword :

                  ReBoot=N    ReBoot=Y      REBOOT=NO       REBOOT=Yes

        UpdateConfig=
                Specify that updating the CONFIG.SYS and SYSTEM.INI
                or not.
                The default setting is Yes, and if the "No" is set,
                updated sample files, named CONFIG.PCM and SYSTEM.PCM
                will be made at target directory.

                Exp. of valid UpdateConfig= keyword :

                  UpdateConfig=N    UpdateConfig=Yes    UPDATECONFIG=NO

        ForceReplace=
                Specify that replacing the PCD files or not, if the
                client workstation has newer dated PCD files.
                The default setting is Yes, and if the "No" is set,
                installation will be terminated.

                Exp. of valid ForceReplace= keyword :

                  ForceReplace=N    ForceReplace=Yes    FORCEREPLACE=NO

        Use2ndSS=
                This keyword is valid only for Win3.1 and DOS on the TP760E
                system. The TP760E needs two SS driver, one for the CardBus
                controller(IBMDSS14), and the other is for the legacy PCIC
                controller(IBMDSS04). This keyword specify that the legacy
                SS driver is enabled or not.
                The default setting is No, and the "DEVICEHIGH=" statement
                for this driver is remed in the CONFIG.SYS

                Exp. of valid Use2ndSS= keyword :

                  Use2ndSS=N    Use2ndSS=Yes    USE2NDSS=NO

