; Future Domain SCSI Card (SCSI2GO)

;* hlp.cardid = Card ID got from Version/Product Information
;* val.port1 = 0x140,0x170
;* hlp.port1 = I/O Port Base Address 1
;* val.port2 = 0
;* hlp.port2 = I/O Port Base Address 2 (Not required)
;* val.irq = 3,5,10,11,12,14,15
;* hlp.irq = Interrupt (IRQ) Level

CardID         =SCSI
FunctionID     =0xFF
ManufacturerID =0x0130
IgnoreCardID   =
EnableSequence =ReqIO(0x140,0xFF,0,0,0,0,0xFF)
                ReqIRQ(0,5)
                ReqConfig(0xFF,0xFF,0xFF,0x08,0,0,0x40)
                IBM_SCSI
                End
DisableSequence=End
