; COMPAQ FDCard

;* hlp.cardid = Card ID got from Version/Product Information
;* hlp.cardid = (This script file is used for COMPAQ AERO.)
;* val.port1 = 0x370,0x3F0
;* hlp.port1 = I/O Port Base Address 1
;* val.port2 = 0
;* hlp.port2 = I/O Port Base Address 2 (Not required)
;* val.irq = 15
;* hlp.irq = Interrupt (IRQ) Level

CardID         =FDCard
FunctionID     =0xFF
ManufacturerID =0xFFFF
IgnoreCardID   =
EnableSequence =ReqIO(0x3F0,0xFF,0,0,0,0,0xFF)
                ReqIRQ(0,15)
                ReqConfig(0xFF,0xFF,0xFF,0x02,0x02,0,0x61)
                End
DisableSequence=End
