; BONDWELL Game card

;* hlp.cardid = Card ID got from Version/Product Information
;* val.port1 = 0x201
;* hlp.port1 = I/O Port Base Address 1
;* val.port2 = 0
;* hlp.port2 = I/O Port Base Address 2 (Not required)

CardID         =B236
FunctionID     =0xFF
ManufacturerID =0x3B01
IgnoreCardID   =
EnableSequence =ReqIO(0x201,0x01,0,0,0,0,0x08)
                ReqConfig(0xFF,0xFF,0xFF,0,0,0,0)
                End
DisableSequence=End
