; IBM PC Card Script File for IBM Auto-Configurator V2.0

Beep           =1000,2,2000,2,800,2,20000,10

; Modem Card (3F8)

;* hlp.cardid = Card ID got from Version/Product Information
;* val.port1 = 0x3F8,0x2F8,0x3E8,0x2E8
;* hlp.port1 = I/O Port Base Address 1
;* val.port2 = 0
;* hlp.port2 = I/O Port Base Address 2 (Not required)
;* val.irq = 3,4
;* hlp.irq = Interrupt (IRQ) Level
;* val.com = 1,2,3,4,0xFF
;* hlp.com = BIOS Data Area Number for COM Number (DOS)/ COM Number (OS/2)

CardID         =MODEM,MD24XC,116E2,118C2,FC2400,2460MC,FC24F,MF0B
FunctionID     =0x02
ManufacturerID =0xFFFF
IgnoreCardID   =SDLC,Serial IR,Sound Card
EnableSequence =ReqIO(0x3F8,0xFF,0,0,0,0,0xFF)
                ReqIRQ(0,4)
                ReqConfig(0xFF,0xFF,0xFF,0x08,0,0,0x40)
                SetupCOM(0xFF)
                End
DisableSequence=DeleteCOM
                End

; Modem Card (2F8)

;* hlp.cardid = Card ID got from Version/Product Information
;* val.port1 = 0x3F8,0x2F8,0x3E8,0x2E8
;* hlp.port1 = I/O Port Base Address 1
;* val.port2 = 0
;* hlp.port2 = I/O Port Base Address 2 (Not required)
;* val.irq = 3,4
;* hlp.irq = Interrupt (IRQ) Level
;* val.com = 1,2,3,4,0xFF
;* hlp.com = BIOS Data Area Number for COM Number (DOS)/ COM Number (OS/2)

CardID         =MODEM,MD24XC,116E2,118C2,FC2400,2460MC,FC24F,MF0B
FunctionID     =0x02
ManufacturerID =0xFFFF
IgnoreCardID   =SDLC,Serial IR,Sound Card
EnableSequence =ReqIO(0x2F8,0xFF,0,0,0,0,0xFF)
                ReqIRQ(0,3)
                ReqConfig(0xFF,0xFF,0xFF,0x08,0,0,0x40)
                SetupCOM(0xFF)
                End
DisableSequence=DeleteCOM
                End

; Modem Card (3E8)

;* hlp.cardid = Card ID got from Version/Product Information
;* val.port1 = 0x3F8,0x2F8,0x3E8,0x2E8
;* hlp.port1 = I/O Port Base Address 1
;* val.port2 = 0
;* hlp.port2 = I/O Port Base Address 2 (Not required)
;* val.irq = 3,4
;* hlp.irq = Interrupt (IRQ) Level
;* val.com = 1,2,3,4,0xFF
;* hlp.com = BIOS Data Area Number for COM Number (DOS)/ COM Number (OS/2)

CardID         =MODEM,MD24XC,116E2,118C2,FC2400,2460MC,FC24F,MF0B
FunctionID     =0x02
ManufacturerID =0xFFFF
IgnoreCardID   =SDLC,Serial IR,Sound Card
EnableSequence =ReqIO(0x3E8,0xFF,0,0,0,0,0xFF)
                ReqIRQ(0,4)
                ReqConfig(0xFF,0xFF,0xFF,0x08,0,0,0x40)
                SetupCOM(0xFF)
                End
DisableSequence=DeleteCOM
                End

; Modem Card (2E8)

;* hlp.cardid = Card ID got from Version/Product Information
;* val.port1 = 0x3F8,0x2F8,0x3E8,0x2E8
;* hlp.port1 = I/O Port Base Address 1
;* val.port2 = 0
;* hlp.port2 = I/O Port Base Address 2 (Not required)
;* val.irq = 3,4
;* hlp.irq = Interrupt (IRQ) Level
;* val.com = 1,2,3,4,0xFF
;* hlp.com = BIOS Data Area Number for COM Number (DOS)/ COM Number (OS/2)

CardID         =MODEM,MD24XC,116E2,118C2,FC2400,2460MC,FC24F,MF0B
FunctionID     =0x02
ManufacturerID =0xFFFF
IgnoreCardID   =SDLC,Serial IR,Sound Card
EnableSequence =ReqIO(0x2E8,0xFF,0,0,0,0,0xFF)
                ReqIRQ(0,3)
                ReqConfig(0xFF,0xFF,0xFF,0x08,0,0,0x40)
                SetupCOM(0xFF)
                End
DisableSequence=DeleteCOM
                End

; IBM SCSI Card

;* hlp.cardid = Card ID got from Version/Product Information
;* val.port1 = 0x140,0x170
;* hlp.port1 = I/O Port Base Address 1
;* val.port2 = 0
;* hlp.port2 = I/O Port Base Address 2 (Not required)
;* val.irq = 3,5,10,11,12,14,15
;* hlp.irq = Interrupt (IRQ) Level

CardID         =SCSI
FunctionID     =0xFF
ManufacturerID =0x00A4
IgnoreCardID   =
EnableSequence =ReqIO(0x140,0xFF,0,0,0,0,0xFF)
                ReqIRQ(0,5)
                ReqConfig(0xFF,0xFF,0xFF,0x08,0,0,0x40)
                IBM_SCSI
                End
DisableSequence=End

End
