; IBM 3270 Card

;* hlp.cardid = Card ID got from Version/Product Information
;* val.port1 = 0x2D0,0x6D0,0xAD0,0xED0
;* hlp.port1 = I/O Port Base Address 1
;* val.port2 = 0
;* hlp.port2 = I/O Port Base Address 2 (Not required)
;* val.irq = 0,1,2,3,4,5,6,7,8,9,10,11,12,13,14,15
;* hlp.irq = Interrupt (IRQ) Level
;* val.window1 = 0xCE000,0xD0000,0xD2000,0xD4000
;* hlp.window1 = Buffer Segment Address
;* val.size1 = 0x2000
;* hlp.size1 = Size of Buffer Segment (8KB)
;* val.offset1 = 0
;* hlp.offset1 = Card Offset for Buffer Segment. It must be 0.

CardID         =3270
FunctionID     =0xFF
ManufacturerID =0x00A4
IgnoreCardID   =
EnableSequence =ReqIO(0x2D0,0x10,0,0,0,0,0xFF)
                ReqIRQ(0,9)
                ReqConfig(0xFF,0xFF,0xFF,0,0,0,0x40)
                ReqWindow(1,0x000C,0xCE000,0x2000,0xFF)
                MapMemPage(1,0)
                End
DisableSequence=End
