[PCIMPA]
 Type       = NDIS_SNGL
 Title      = IBM PCI Multiprotocol Adapter MAC
 Version    = 1.0
 DriverName = PCIMPA$
 NoBind     = Yes

[FILE]
 Name = PCIMPADD.SYS
 Path = \IBMCOM\MACS

[PORTNAME]
 Display  = "Portname"
 Type     = String
 StrLength = 16
 Optional = No
 Editable = Yes
 Help     = "The port name creates a logical identifier for the physical
 hardware port so the Port Connection Manager(PCM) subsystem can reference
 the port. All port names defined in the system must be unique.
 The value specifed can be anything except MPA0 and MPA1 which are reserved
 for MPADD.SYS which supports the ISA and MCA MPA adapters.
 This name must match the port name specified in the PCM
 configuration in Communication Server/2 or Access Feature."

[CONSTANT_RTS]
 Display  = "Constant RTS"
 Type     = String
 StrLength = 16
 Default   = "YES"
 Set       = "YES","NO"
 Optional = Yes
 Editable = Yes
 Help     = "This indicates whether hardware flow control is used between the
 adapter and the modem.
 If this is set to YES, Request to Send(RTS) and Clear to Send(CTS) are
 always asserted and no hardware flow control is used.
 If this is set to NO, hardware flow control is used. When
 the adapter has data to transmit, RTS is asserted and the adapter waits
 until the modem asserts CTS before sending any data.
 This parameter should be set to NO when this station is a secondary link
 station on a multidrop line."

[ADAPTERNUMBER]
 Display  = "Adapter number"
 Type     = DecNum
 Default  = 0
 Range    = 0-1
 Optional = No
 Editable = Yes
 Help     = "Identifies the physical IBM PCI Multiprotocol adapter (MPA) card
 in the system.  For
 systems with a single PCI MPA adapter card, this value must be 0.  For systems
 with multiple PCI MPA adapter cards, adapter number 0 will be the first
 PCI MPA adapter
 that the system finds and adapter number 1 will be the second adapter
 found."
