*
*
*
*+-------------------------------------------------------------------+
*                                                                   
* DATE: 10/25/00
*                                                                   
* DESCRIPTION:   This APAR provides IBM Communications Server/2  and
*                IBM OS/2 Access Feature versions 5.X and 6.X
*                 with a driver for the PCI MPA
*                adapter XXXXXXX (FRU XXXXXXXX).
*                                                                   
* README FILE FOR  IBM OS/2 Access Feature for OS/2 Warp 
*                   and IBM Communications Server/2 for OS/2 WARP 
*                  Versions 5.X and 6.X
*                                                                   
* APAR: JR14426
*                                                                   
*                                                                   
* This package contains APAR fixes to the product above.  This      
* package can be distributed to any one who has a license for       
* this product.                                                     
*                                                                   
*+-------------------------------------------------------------------+
*
*
* PREREQUISITES :   IBM OS/2 Access Feature for OS/2 Warp 
*                   and IBM Communications Server/2 for OS/2 WARP 
*
* PROBLEMS FIXED:  JR14426   Provides support for New PCI MPA adapter.
*
*
* 
* FILES PROVIDED   PCIMAPDD.SYS
*                  PCIMPADD.NIF 
*
* INSTALLATION INSTRUCTIONS:
*
* NOTE: If adapter is ALREADY installed, rename the existing files to
*	*.OLD and replace with the new files in the
*       <install drive>:\IBMCOM\MACS directory. Nothing further should be
*         required.
*
*  If adapter has never been installed, verify that the above mentioned
*  files are not present on your machine, If they are, replace them,
*  after renaming them to *.OLD,and then continue.
*  You must first install this driver through MPTS and then add it to
*  your Current Configuration.  Next, hilite the "IBM PCI 
*  Multiprotocol Adapter MAC" in your Current Configuration and select
*  Edit.  There are 3 fields that need to be set:
*
*  Portname : Input a unique string that will identify this port.  It
*  can be any value except MPA0 or MPA1 which are reserved for another
*  driver.  When you configure the PCM configuration in Communication
*  Server/2 or Access Feature, the port name there must match the
*  portname defined in this panel.  (Note: if more than one IBM PCI
*  Multiprotocol Adapter is installed in a system, each adapter must
*  have a unique Portname).
*
*  Constant RTS : This parameter should be set to NO when this station
*  is a secondary link station on a multidrop line."
*
*  Adapter number :  If there is only one IBM PCI Multiprotocol 
*  adapter in the system, this must be a 0.  If there are two of these
*  adapters in the system, one adapter will be adapter number 0 and 
*  the other will be adapter number 1.
*
*  Next, type CMSETUP at a command line.  During the Port Connection
*  Manager Configuration, you must select the "Synchronous Leased Line
*  Modem(WAC,OEM)" or "Synchronous Switched Modem (WAC,OEM)" to 
*  perform the configuration.  Do not select the MPA entries.
*
*
*+-------------------------------------------------------------------+
*
*
* CONTACT FOR SUPPORT:
*
*   If you have any questions, please call the IBM SUPPORT CENTER
*   for your Country.  For example in the USA call: 1-800-237-5511
*
*
*
* IBM COPYRIGHT INFORMATION:
*
*   IBM OS/2 Access Feature for OS/2 Warp 
*
*   Copyright International Business Machines Corporation 1989, 1997. All
*   rights reserved.  Note to U.S. Government Users - Documentation
*   related to restricted rights - Use, duplication or disclosure is
*   subject to restrictions set forth in GSA ADP Schedule Contract
*   with IBM Corp.
*
*
**
*
* LIMIT OF LIABILITY:
*
*   License to the contained APAR fixes is conditioned upon the recipient
*   holding a license to the prerequisite product.  The license terms
*   and conditions of the APAR fixes are the same as those for the
*   prerequisite product.  Please see the product license for specifics.
*
*******************************************************************************
