; SafeFire Links requires this device driver
; to communicate with TCP/IP stack and simulate lanXX interfaces.

[SFMAC]
 Type = NDIS
 Title = "SafeFire Links MAC Driver"
 Version = 1.1.6
 DriverName = SFMAC$
 XPORTS = NETBEUI, LANDD
 Nobind=Yes

[File]
 Name = SFMAC.SYS
 Path = \IBMCOM\MACS

[netaddress]
 Display = "Network address"
 Type = HexString
 StrLength = 12
 Optional = Yes
 Editable = Yes
 Help = "This parameter overrides the network address automatically
         detected by driver. The value of this parameter is a string
         of 12 hexadecimal digits of the address. Address must be
         the same as real MAC adapter address."
