## SafeFire Links

### v1.3a

# Installation Guide

To install SafeFire Links you need to perform following steps:

1. Unpack SafeFire Links archive file into the directory where you want to run it.

2. Run install.cmd and follow directions.

3. If PPPoE (PPP over Ethernet) support is required then refer to PPP over Ethernet Configuration Guide for details of NDIS driver setup.

4. Restart your computer if required.

5. For command line version of software:

   1. Choose appropriate configuration file and alter it to accommodate your settings (see "Up and running" book).

   2. Run SafeFire Links CLI using the following command:

          sfcli -Cconfig_file_name

6. For GUI version of software:

   1. Run sfgui.exe.

   2. Click on Configure button.

   3. On the first page of settings select appropriate scenario.
      For example, if it is planned to use dial-up connection over ordinary phone line and share connection with other PC's in the LAN you may choose one of the following scenarios:
      - Dial-up client with NAT, DOD and a filter
      - Dial-up client with NAT, DOD and 3 filters

   4. On Connection page of settings fill User ID and Password entry fields.
      For serial connection (ISDN, dial-up or leased line) check and update if required Modem port and Port speed fields.
      For all serial connection types except leased line connection Phone field is required too.

      NOTE: Only port names COM1 thru COM8 are listed in Modem port combo box. If other port is needed then just type port name there.
      For example, if SafeFire Links should use COM port shared on the server SERVER1 as SERIAL1 on the other OS/2 PC in the LAN then just type full name to the shared port resource:

          \\SERVER1\SERIAL1

   5. If it is desired to allow GUI to save password in INI file - check Remember check box.

   6. For serial connections on Advanced page of settings dialog Modem init string and Dial prefix entry fields may require adjustment.

   7. Sample dnshook.cmd script coming with SafeFire Links package maintain DNS information provided by ISP and received during PPP connection setup. It is recommended to update script settings by clicking on REXX -> Configure push button.
      If local DNS server is installed or it is not desired to to allow SafeFire Links to maintain DNS information then just clear REXX Script field.

   8. Click on Ok push button.

   9. After closing of Settings dialog, Configure push button will change its name to Connect. Click on it and SafeFire Links will start establishing of connection.

Return to documentation index | SafeFire Links (C) Link Guard Solutions 1999, 2000