Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES

## Package com.sun.management.oss.pm.opstatus

This package refers to systems capabilities to read operational status of observed managed object(s) (MBeans) and to produce status reports when status changes occur.

See:
Description

Interface Summary
CurrentResultReport | This interface represents report of the current values of a measurement job.
JVTOperationalStatusMonitorSession | The JVTOperationalStatusMonitorSession interface is the central interface of this package to manage measurement jobs.
JVTOperationalStatusMonitorSessionOptionalOpt | This interface defines string constants to indicate which optional parts of the `JVTOperationalStatusMonitorSession` interface that are supported by an implementation.
OperationalStatusAttributeDescriptor | Represent a measurement attribute that can be monitored in the observable object class.
OperationalStatusDataAvailableEvent | This interface represents the payload of the event that is sent when a measurement report file has been created.
OperationalStatusDataAvailableEventDescriptor | The `OperationalStatusDataAvailableEventDescriptor` interface is equivalent to an enumerated type.
OperationalStatusDataEvent | The performance data event defines the payload of the events that contains measurement reports.
OperationalStatusDataEventDescriptor | The `OperationalStatusDataEventDescriptor` interface is equivalent to an enumerated type.
OperationalStatusMonitorByClassesValue | This interface is the value representation of a measurement job that monitor a set of specified attributes on a set of observable object classes.
OperationalStatusMonitorByObjectsValue | This interface is the value representation of a measurement job that monitor a set of specified attributes on a set of observable object instances.
OperationalStatusMonitorKey | This interface is the primary key of a performance monitor instance.
OperationalStatusMonitorKeyResult | This interface encapsulates all the information necessary to indicate the result of a BEST EFFORT operation on a specific measurement job.
OperationalStatusMonitorState | Defines the state constants for performance monitor.
OperationalStatusMonitorValue | This interface is the base value representation of a measurement job.
OperationalStatusMonitorValueIterator | This interface manages retrieval of multiple measurement jobs.
QueryByDNValue | This interface is used to query for measurement jobs by specifying distinguished names.
QueryOperationalStatusMonitorValue | This interface represents the attributes of a measurement job that can be used to make queries for measurement jobs.
ReportData | This interface represents the measurement reports.
ReportFormat | This interface represent the format of the measurements reports.
ReportInfo | Contains information related to a measurement report file.
ReportInfoIterator | This interface manages retrieval of information for multiple measurement reports.
ReportMode | Defines enumeration values for report mode.

## Package com.sun.management.oss.pm.opstatus Description

This package refers to systems capabilities to read operational status of observed managed object(s) (MBeans) and to produce status reports when status changes occur.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
PREV PACKAGE NEXT PACKAGE | FRAMES NO FRAMES