# Setting Up DR-WebSpyder For the First Time When you installed DR-WebSpyder, you will have either chosen to use a modem connection or a LAN connection. If you need to change from a LAN connection to a modem or vice versa after you have installed DR-WebSpyder, you will need to re-install DR-WebSpyder.
1. | When you have installed DR-WebSpyder and restarted your computer, you start DR-WebSpyder by entering the following in the directory you installed it. DRWEBSPY
| The screen resolution setup page is displayed.
2. | Choose the resolution you need such as Autodetect;800x600;15bbp colors, then click OK to start DR-WebSpyder.
| DR-WebSpyder starts and displays the first setup page. This shows how you are connecting to the Internet: either Dial-up or LAN. You can click on the Next button to continue.
| Follow the screens and enter the information requested.
3. | Click the Finish button.
| Your settings are saved and you are returned to the Setup Menu. You can then setup other DR-WebSpyder settings such as E-mail settings or your home and searh pages.
Refer to "Connecting to the Internet" for more information. Return to Help Contents