
                                    FYI

(Note: The origin of this information may be internal or external
to Novell.  Novell makes every effort within its means to verify
this information.  However, the information provided in this
document is FOR YOUR INFORMATION only.  Novell makes no explicit or
implied claims to the validity of this information.)

          TITLE: Digichannel PC/4
   DOCUMENT ID#: FYI-M-1910
           DATE: 08-04-92
        PRODUCT: Multiuser DOS
PRODUCT VERSION: 5.0, 5.1
     SUPERSEDES:

ISSUE/PROBLEM
The recommended settings for the board are as follows:

IRQ 3
Base Address 100
Status Register 140

Setting up DR Multiuser DOS:

After installing the physical PC/4 board into the machine, run
SETUP, and enable the "DigiBoard" multiport driver.  Exit SETUP.

Using EDITOR, modify the file DRMDOS.INP.  This is located on the
root directory of the primary hard disk drive partition.  Find the
section labeled "setmulti" and change the value of "nports=" from
"8" to "4".  Save the file, and exit EDITOR.

Finally, run SETUP /I DRMDOS.SYS DRMDOS.INP to update the DRMDOS
system file with the new information, and reboot.  If DR Multiuser
DOS is the only operating system on the hard disk, replace
DRMDOS.SYS with IBMDOS.COM in the instruction above.
