
                                    FYI

(Note: The origin of this information may be internal or external to Novell.  Novell makes every effort within its means to verify this information.  However, the information provided in this document is FOR YOUR INFORMATION only.  Novell makes no explicit or implied claims to the validity of this information.)

          TITLE: Arnet Multiport Card
   DOCUMENT ID#: FYI-M-1999
           DATE: 07-07-92
        PRODUCT: Arnet
PRODUCT VERSION:
     SUPERSEDES:

SOLUTION

                   ARNET MULTIPORT CARD


When using this multiport card, please note that the documentation on switch settings in the manual is incorrect. Appendix C, page 4 should be as follows:

Address 280H
IRQ 3
Option Address 270H

SW1 1, 2, 4 - ON    SW2 1, 5, 6    - ON    SW3     2       - ON 
    3, 5    - OFF       2, 3, 4, 7 - OFF     1, 3, 4, 5, 6 - OFF

Alternative:-

Address 2C0H
IRQ 3
Option Address 2B0H

SW1 1, 2    - ON    SW2 1, 4, 6    - ON    SW3     2       - ON 
    3, 4, 5 - OFF       2, 3, 5, 7 - OFF     1, 3, 4, 5, 6 - OFF
