

NOVELL TECHNICAL INFORMATION DOCUMENT

DOCUMENT PROCESSING INFO:  This Document replaces FYI-M-1618
TITLE:  Configuring AutoCAD rel. 11
DOCUMENT ID:  TID800045
DOCUMENT REVISION:  A
DATE:  17AUG94
AUTHOR:  DBADGER;DPARTRID
ALERT STATUS:  Yellow
DISTRIBUTION:  Public
INFORMATION TYPE:  Symptom Solution
README FOR:  NA
NOVELL PRODUCT CLASS:

Desktop Products

NOVELL PRODUCT and VERSION:

DR DOS 6.0

CATEGORY:

Compression

ABSTRACT:

NA

-----------------------------------------------------------------
DISCLAIMER
THE ORIGIN OF THIS INFORMATION MAY BE INTERNAL OR EXTERNAL TO
NOVELL.  NOVELL MAKES EVERY EFFORT WITHIN ITS MEANS TO VERIFY THIS
INFORMATION.  HOWEVER, THE INFORMATION PROVIDED IN THIS DOCUMENT
IS FOR YOUR INFORMATION ONLY.  NOVELL MAKES NO EXPLICIT OR IMPLIED
CLAIMS TO THE VALIDITY OF THIS INFORMATION.
-----------------------------------------------------------------

SYMPTOM

AutoCad VMM Errors similar to:

EAX=005E0040 EBX=02000000
LINADR=00E7B000
Fatal Error 386 | VMM:
Bad Page table entry in PG FLT HNDLR

CAUSE

If the AutoCAD swap file is created on a SuperStor compressed
partition, it is given maximum compression ratio of 16:1.  When
AutoCAD then creates other working files on the compressed
partition, they prevent the swap file from expanding as necessary,
resulting in an error from the Virtual Memory Manager (VMM).

SOLUTION

SOLUTION
Create the AutoCAD swap file on an uncompressed partition.  Users
ought to refer to their AutoCAD documentation for instructions on
this.  Here are the steps that we have found to work:


1) Execute a configuration program called CFIG386.EXE.  The
necessary command is: CFIG386 ACAD.EXE -SWAPDEFDISK x:  (where x:
is the drive designation of the uncompressed partition).

2) It is also possible to designate a directory in which the file
should reside by entering:  CFIG386 ACAD.EXE -SWAPDIR x:\temp
(where x:\temp is the drive and directory on the uncompressed
partition).

There needs to be about 5 Megabytes of free disk space on the
uncompressed partition before CFIG386 can make these changes.  If
this is not the case, it will be necessary to backup the data on
the compressed partition, remove the compressed partition, and
recreate it, leaving the uncompressed partition about 5 MB larger
than it currently is.

Other configuration tips regarding AutoCAD 11 are as follows:
(1) set FILES=100
(2) set FCBS=48,8
(3) set BREAK=OFF.
These changes are to the CONFIG.SYS file.

KeyWords DR6 Autocad VMM swapfile

-----------------------------------------------------------------
Any trademarks referenced in this document are the property of their respective owners. 
Consult your product manuals for complete trademark information.
-----------------------------------------------------------------
