ATA.SYS - PCMCIA ATA disk driver v1.1                  12-17-96
Copyright (c) 1996-2001 Datalight, Inc.


Usage: ATA.SYS [/AXXXX] [/IXXXX]
  /AXXXX     Replace XXXX with the memory segment to use
               Defaults to CC00
  /IXXXX     Replace XXXX with the IO address to use
               Defaults to 240

Requires an Intel 82365 or compatible controller.
Only supports 5 volt ATA cards.
Supports up to 2 drives.
Use ROM-DOS FORMAT to format an ATA disk, if not already formatted.
Fully hot-swappable.

ATA Cards tested:
  Integral 1841PA 17MB ATA card  660KB/s write, 690KB/s read
  Toshiba TH6SS160201AA 20MB ATA card 900KB/s write, 1200KB/s read
  SanDisk SDCFB 4MB CompactFlash card 300KB/s write, 1000KB/s read
  SanDisk SDP3B 2MB ATA card 275KB/s writem 1000KB/s read

Controllers tested:
  Vadem VG-465
  Intel 82365SL rev A
