Go to the first, previous, next, last section, table of contents.

# Passes and Files of the Compiler

The overall control structure of the compiler is in ``toplev.c'`. This file is responsible for initialization, decoding arguments, opening and closing files, and sequencing the passes.

The parsing pass is invoked only once, to parse the entire input. The RTL intermediate code for a function is generated as the function is parsed, a statement at a time. Each statement is read in as a syntax tree and then converted to RTL; then the storage for the tree for the statement is reclaimed. Storage for types (and the expressions for their sizes), declarations, and a representation of the binding contours and how they nest, remain until the function is finished being compiled; these are all needed to output the debugging information.

Each time the parsing pass reads a complete function definition or top-level declaration, it calls either the function `rest_of_compilation`, or the function `rest_of_decl_compilation` in ``toplev.c'`, which are responsible for all further processing necessary, ending with output of the assembler language. All other compiler passes run, in sequence, within `rest_of_compilation`. When that function returns from compiling a function definition, the storage used for that function definition's compilation is entirely freed, unless it is an inline function (see section An Inline Function is As Fast As a Macro).

Here is a list of all the passes of the compiler and their source files. Also included is a description of where debugging dumps can be requested with ``-d'` options.

- Parsing. This pass reads the entire text of a function definition, constructing partial syntax trees. This and RTL generation are no longer truly separate passes (formerly they were), but it is easier to think of them as separate. The tree representation does not entirely follow C syntax, because it is intended to support other languages as well. Language-specific data type analysis is also done in this pass, and every tree node that represents an expression has a data type attached. Variables are represented as declaration nodes. Constant folding and some arithmetic simplifications are also done during this pass. The language-independent source files for parsing are ``stor-layout.c'`, ``fold-const.c'`, and ``tree.c'`. There are also header files ``tree.h'` and ``tree.def'` which define the format of the tree representation. The source files to parse C are ``c-parse.in'`, ``c-decl.c'`, ``c-typeck.c'`, ``c-aux-info.c'`, ``c-convert.c'`, and ``c-lang.c'` along with header files ``c-lex.h'`, and ``c-tree.h'`. The source files for parsing C++ are ``cp-parse.y'`, ``cp-class.c'`,
  ``cp-cvt.c'`, ``cp-decl.c'`, ``cp-decl2.c'`, ``cp-dem.c'`, ``cp-except.c'`,
  ``cp-expr.c'`, ``cp-init.c'`, ``cp-lex.c'`, ``cp-method.c'`, ``cp-ptree.c'`,
  ``cp-search.c'`, ``cp-tree.c'`, ``cp-type2.c'`, and ``cp-typeck.c'`, along with header files ``cp-tree.def'`, ``cp-tree.h'`, and ``cp-decl.h'`. The special source files for parsing Objective C are ``objc-parse.y'`, ``objc-actions.c'`, ``objc-tree.def'`, and ``objc-actions.h'`. Certain C-specific files are used for this as well. The file ``c-common.c'` is also used for all of the above languages.
- RTL generation. This is the conversion of syntax tree into RTL code. It is actually done statement-by-statement during parsing, but for most purposes it can be thought of as a separate pass. This is where the bulk of target-parameter-dependent code is found, since often it is necessary for strategies to apply only when certain standard kinds of instructions are available. The purpose of named instruction patterns is to provide this information to the RTL generation pass. Optimization is done in this pass for `if`-conditions that are comparisons, boolean operations or conditional expressions. Tail recursion is detected at this time also. Decisions are made about how best to arrange loops and how to output `switch` statements. The source files for RTL generation include ``stmt.c'`, ``calls.c'`, ``expr.c'`, ``explow.c'`, ``expmed.c'`, ``function.c'`, ``optabs.c'` and ``emit-rtl.c'`. Also, the file ``insn-emit.c'`, generated from the machine description by the program `genemit`, is used in this pass. The header file ``expr.h'` is used for communication within this pass. The header files ``insn-flags.h'` and ``insn-codes.h'`, generated from the machine description by the programs `genflags` and `gencodes`, tell this pass which standard names are available for use and which patterns correspond to them. Aside from debugging information output, none of the following passes refers to the tree structure representation of the function (only part of which is saved). The decision of whether the function can and should be expanded inline in its subsequent callers is made at the end of rtl generation. The function must meet certain criteria, currently related to the size of the function and the types and number of parameters it has. Note that this function may contain loops, recursive calls to itself (tail-recursive functions can be inlined!), gotos, in short, all constructs supported by GNU CC. The file ``integrate.c'` contains the code to save a function's rtl for later inlining and to inline that rtl when the function is called. The header file ``integrate.h'` is also used for this purpose. The option ``-dr'` causes a debugging dump of the RTL code after this pass. This dump file's name is made by appending ``.rtl'` to the input file name.
- Jump optimization. This pass simplifies jumps to the following instruction, jumps across jumps, and jumps to jumps. It deletes unreferenced labels and unreachable code, except that unreachable code that contains a loop is not recognized as unreachable in this pass. (Such loops are deleted later in the basic block analysis.) It also converts some code originally written with jumps into sequences of instructions that directly set values from the results of comparisons, if the machine has such instructions. Jump optimization is performed two or three times. The first time is immediately following RTL generation. The second time is after CSE, but only if CSE says repeated jump optimization is needed. The last time is right before the final pass. That time, cross-jumping and deletion of no-op move instructions are done together with the optimizations described above. The source file of this pass is ``jump.c'`. The option ``-dj'` causes a debugging dump of the RTL code after this pass is run for the first time. This dump file's name is made by appending ``.jump'` to the input file name.
- Register scan. This pass finds the first and last use of each register, as a guide for common subexpression elimination. Its source is in ``regclass.c'`.
- Jump threading. This pass detects a condition jump that branches to an identical or inverse test. Such jumps can be ``threaded'` through the second conditional test. The source code for this pass is in ``jump.c'`. This optimization is only performed if ``-fthread-jumps'` is enabled.
- Common subexpression elimination. This pass also does constant propagation. Its source file is ``cse.c'`. If constant propagation causes conditional jumps to become unconditional or to become no-ops, jump optimization is run again when CSE is finished. The option ``-ds'` causes a debugging dump of the RTL code after this pass. This dump file's name is made by appending ``.cse'` to the input file name.
- Loop optimization. This pass moves constant expressions out of loops, and optionally does strength-reduction and loop unrolling as well. Its source files are ``loop.c'` and ``unroll.c'`, plus the header ``loop.h'` used for communication between them. Loop unrolling uses some functions in ``integrate.c'` and the header ``integrate.h'`. The option ``-dL'` causes a debugging dump of the RTL code after this pass. This dump file's name is made by appending ``.loop'` to the input file name.
- If ``-frerun-cse-after-loop'` was enabled, a second common subexpression elimination pass is performed after the loop optimization pass. Jump threading is also done again at this time if it was specified. The option ``-dt'` causes a debugging dump of the RTL code after this pass. This dump file's name is made by appending ``.cse2'` to the input file name.
- Stupid register allocation is performed at this point in a nonoptimizing compilation. It does a little data flow analysis as well. When stupid register allocation is in use, the next pass executed is the reloading pass; the others in between are skipped. The source file is ``stupid.c'`.
- Data flow analysis (``flow.c'`). This pass divides the program into basic blocks (and in the process deletes unreachable loops); then it computes which pseudo-registers are live at each point in the program, and makes the first instruction that uses a value point at the instruction that computed the value. This pass also deletes computations whose results are never used, and combines memory references with add or subtract instructions to make autoincrement or autodecrement addressing. The option ``-df'` causes a debugging dump of the RTL code after this pass. This dump file's name is made by appending ``.flow'` to the input file name. If stupid register allocation is in use, this dump file reflects the full results of such allocation.
- Instruction combination (``combine.c'`). This pass attempts to combine groups of two or three instructions that are related by data flow into single instructions. It combines the RTL expressions for the instructions by substitution, simplifies the result using algebra, and then attempts to match the result against the machine description. The option ``-dc'` causes a debugging dump of the RTL code after this pass. This dump file's name is made by appending ``.combine'` to the input file name.
- Instruction scheduling (``sched.c'`). This pass looks for instructions whose output will not be available by the time that it is used in subsequent instructions. (Memory loads and floating point instructions often have this behavior on RISC machines). It re-orders instructions within a basic block to try to separate the definition and use of items that otherwise would cause pipeline stalls. Instruction scheduling is performed twice. The first time is immediately after instruction combination and the second is immediately after reload. The option ``-dS'` causes a debugging dump of the RTL code after this pass is run for the first time. The dump file's name is made by appending ``.sched'` to the input file name.
- Register class preferencing. The RTL code is scanned to find out which register class is best for each pseudo register. The source file is ``regclass.c'`.
- Local register allocation (``local-alloc.c'`). This pass allocates hard registers to pseudo registers that are used only within one basic block. Because the basic block is linear, it can use fast and powerful techniques to do a very good job. The option ``-dl'` causes a debugging dump of the RTL code after this pass. This dump file's name is made by appending ``.lreg'` to the input file name.
- Global register allocation (``global.c'`). This pass allocates hard registers for the remaining pseudo registers (those whose life spans are not contained in one basic block).
- Reloading. This pass renumbers pseudo registers with the hardware registers numbers they were allocated. Pseudo registers that did not get hard registers are replaced with stack slots. Then it finds instructions that are invalid because a value has failed to end up in a register, or has ended up in a register of the wrong kind. It fixes up these instructions by reloading the problematical values temporarily into registers. Additional instructions are generated to do the copying. The reload pass also optionally eliminates the frame pointer and inserts instructions to save and restore call-clobbered registers around calls. Source files are ``reload.c'` and ``reload1.c'`, plus the header ``reload.h'` used for communication between them. The option ``-dg'` causes a debugging dump of the RTL code after this pass. This dump file's name is made by appending ``.greg'` to the input file name.
- Instruction scheduling is repeated here to try to avoid pipeline stalls due to memory loads generated for spilled pseudo registers. The option ``-dR'` causes a debugging dump of the RTL code after this pass. This dump file's name is made by appending ``.sched2'` to the input file name.
- Jump optimization is repeated, this time including cross-jumping and deletion of no-op move instructions. The option ``-dJ'` causes a debugging dump of the RTL code after this pass. This dump file's name is made by appending ``.jump2'` to the input file name.
- Delayed branch scheduling. This optional pass attempts to find instructions that can go into the delay slots of other instructions, usually jumps and calls. The source file name is ``reorg.c'`. The option ``-dd'` causes a debugging dump of the RTL code after this pass. This dump file's name is made by appending ``.dbr'` to the input file name.
- Conversion from usage of some hard registers to usage of a register stack may be done at this point. Currently, this is supported only for the floating-point registers of the Intel 80387 coprocessor. The source file name is ``reg-stack.c'`. The options ``-dk'` causes a debugging dump of the RTL code after this pass. This dump file's name is made by appending ``.stack'` to the input file name.
- Final. This pass outputs the assembler code for the function. It is also responsible for identifying spurious test and compare instructions. Machine-specific peephole optimizations are performed at the same time. The function entry and exit sequences are generated directly as assembler code in this pass; they never exist as RTL. The source files are ``final.c'` plus ``insn-output.c'`; the latter is generated automatically from the machine description by the tool ``genoutput'`. The header file ``conditions.h'` is used for communication between these files.
- Debugging information output. This is run after final because it must output the stack slot offsets for pseudo registers that did not get hard registers. Source files are ``dbxout.c'` for DBX symbol table format, ``sdbout.c'` for SDB symbol table format, and ``dwarfout.c'` for DWARF symbol table format.

Some additional files are used by all or many passes:

- Every pass uses ``machmode.def'` and ``machmode.h'` which define the machine modes.
- Several passes use ``real.h'`, which defines the default representation of floating point constants and how to operate on them.
- All the passes that work with RTL use the header files ``rtl.h'` and ``rtl.def'`, and subroutines in file ``rtl.c'`. The tools `gen*` also use these files to read and work with the machine description RTL.
- Several passes refer to the header file ``insn-config.h'` which contains a few parameters (C macro definitions) generated automatically from the machine description RTL by the tool `genconfig`.
- Several passes use the instruction recognizer, which consists of ``recog.c'` and ``recog.h'`, plus the files ``insn-recog.c'` and ``insn-extract.c'` that are generated automatically from the machine description by the tools ``genrecog'` and ``genextract'`.
- Several passes use the header files ``regs.h'` which defines the information recorded about pseudo register usage, and ``basic-block.h'` which defines the information recorded about basic blocks.
- ``hard-reg-set.h'` defines the type `HARD_REG_SET`, a bit-vector with a bit for each hard register, and some macros to manipulate it. This type is just `int` if the machine has few enough hard registers; otherwise it is an array of `int` and some of the macros expand into loops.
- Several passes use instruction attributes. A definition of the attributes defined for a particular machine is in file ``insn-attr.h'`, which is generated from the machine description by the program ``genattr'`. The file ``insn-attrtab.c'` contains subroutines to obtain the attribute values for insns. It is generated from the machine description by the program ``genattrtab'`.

Go to the first, previous, next, last section, table of contents.