InS_StArT
E935.COM
1.0
^CNet CN935 PCI Bus Ethernet Adapter,E935.COM,0E0
?PCI hardware configuration is auto-selected by BIOS
$O0E0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*O0E0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!O0E0()Media Access Type
?NOTE: Media access type will be autodetected on driver's load
TP
TP_NO_LINK_TEST
TP_FULL_DUPLEX
BNC
@AUTOSENSE
InS_EnD
