InS_StArT
EN32VL.COM
1.0
^Compex ENET32-VL,EN32VL.COM,I00
!OI00(BUSTYPE)Bus Type
@VESA
!OI00(PORT)Base I/O Port
?You can specify the I/O port address, or let the driver scan for you.
220
240
280
2A0
300
320
340
380
!OI00()Optional Keyword
TP
$OI00(NODE ADDRESS)Optional Node Address
0
7FFFFFFFFFFF
*RI00(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
