InS_StArT
ENETCPSH.COM
1.0
^Compex ENET P-Series adapters,ENETCPSH.COM,IEM,70DE
!OIE0 (MODE) Driver Configuration Mode
?Select the driver configuration mode for your network adapter.
@AUTO
PROGRAM
!RIE0 (MEDIA) Cable Type
?Select the physical media.
AUI
@BNC
TPI
!OIE0 (PORT) I/O Base Port
?For MODE AUTO, this entry is ignored. For MODE PROGRAM, please select an I/O Base Port to be programmed.
200
220
240
260
280
2A0
2C0
2E0
300
320
340
360
380
3A0
3C0
3E0
!O00M (SLOT) Microchannel Slot
1
2
3
4
5
6
7
8
!OIE0 (INT) Hardware Interrupt
?For MODE AUTO, this entry is ignored. For MODE PROGRAM, please select an interrupt level to be programmed.
2
3
4
5
7
10
11
14
15
!OIE0 (MEM) Memory Address
?For MODE AUTO, this entry is ignored. For MODE PROGRAM, please select a memory address to be programmed.
c0000
c2000
c4000
c6000
c8000
ca000
cc000
ce000
d0000
d2000
d4000
d6000
d8000
da000
dc000
de000
e0000
e2000
e4000
e6000
e8000
ea000
ec000
ee000
!OIEM (NODE ADDRESS) Optional Node Address
0
7FFFFFFFFFFF
*RIEM (FRAME) Frame Types
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
