f c:\tiga\tigacd.exe ^tigaerr
T0 TIGA AutoCAD Driver Installation 
^top
z
|Select the item you wish to install and press Enter, or type the number.
|
S1 TIGA AutoCAD Release  9 Driver Installation 
S2 TIGA AutoCAD Release 10 Driver Installation 
S3 TIGA AutoCAD Release 11 Driver Installation 
S4 Quit
W0 
z
e %0 1 ^acad9
e %0 2 ^acad10
e %0 3 ^acad11
e %0 4 ^quit
j ^top

^acad9
=1ACAD9
=49
=8N
=9N
j ^JOB

^acad10
=1ACAD10
=410
j ^ASK

^acad11
=1ACAD11
=411
j ^ASK

^ASK
z
|Which language do you wish to use for AutoCAD ?
|
|      1. English
|      2. German
|      3. French
|
=81
@8Type a number (1-3): 
e %8 esc ^top
e "%8" "" ^top
z
|Do you wish to install the ADI protect mode (P386) driver ?
|
=9N
@9Y/N: 
e %9 esc ^top
e "%9" "" ^top
j ^JOB

^JOB
z
e %8 2 ^g1
e %8 3 ^f1
T0 Installing TIGA AutoCAD Release %4 Driver 
j ^e1

^f1
T0 Installing TIGA AutoCAD Release %4 (French) Driver 
j ^e1
^g1
T0 Installing TIGA AutoCAD Release %4 (German) Driver 
^e1
Di0
j ^wf

^hnotf
z
|Invalid target drive and directory specification
|
!Hit any key to return.
^wf
z
|Type the target drive to copy the ADI driver to.
|
=7C
@7Target Drive (C-Z): 
e %7 esc ^top
e "%7" "" ^top
z
|Type the target directory to copy the ADI driver to.
|
=5\%1
@5Target Directory : 
z
e %5 esc ^wf
f %7:%5\acad.exe ^hnotf
z
e %1 ACAD10 ^job10
e %1 ACAD11 ^job11

^job9
c %0\ACAD9\ADIEXT.RLM C:\TIGA ^cerr
c %0\ACAD9\ADI.EXE %7:%5 ^cerr
z
|This concludes the installation of TIGA AutoCAD Release %4 Driver.
|Change to the directory %7:%5 and run ADI.EXE before running AutoCAD.
|
j ^finish

^job10
e %9 y ^p10
=6DSTIG40
=2V4.0
c %0\acad10\dstig40.exe %7:%5 ^cerr
c %0\acad10\adicfg.exe %7:%5 ^cerr
c %0\acad10\dstig40.rlm c:\tiga ^cerr
e %8 2 ^r10g
e %8 3 ^r10f
c %0\acad10\dstig40.uk %7:%5\DSTIG40.CMD ^cerr
j ^common
^r10g
c %0\acad10\dstig40.gr %7:%5\DSTIG40.CMD ^cerr
j ^common
^r10f
c %0\acad10\dstig40.fr %7:%5\DSTIG40.CMD ^cerr
j ^common
^p10
=6DSPTIG40
=2V4.0
c %0\acad10\dsptig40.exp %7:%5 ^cerr
c %0\acad10\dsptig40.rlm c:\tiga ^cerr
e %8 2 ^p10g
e %8 3 ^p10f
c %0\acad10\dsptig40.uk %7:%5\DSPTIG40.CMD ^cerr
j ^common
^p10g
c %0\acad10\dsptig40.gr %7:%5\DSPTIG40.CMD ^cerr
j ^common
^p10f
c %0\acad10\dsptig40.fr %7:%5\DSPTIG40.CMD ^cerr
j ^common

^job11
e %9 y ^p11
=6DSTIG41
=2V4.1
c %0\acad11\dstig41.exe %7:%5 ^cerr
c %0\acad11\adicfg.exe %7:%5 ^cerr
c %0\acad11\dstig41.rlm c:\tiga ^cerr
e %8 2 ^r11g
e %8 3 ^r11f
c %0\acad11\dstig41.uk %7:%5\DSTIG41.CMD ^cerr
j ^common
^r11g
c %0\acad11\dstig41.gr %7:%5\DSTIG41.CMD ^cerr
j ^common
^r11f
c %0\acad11\dstig41.fr %7:%5\DSTIG41.CMD ^cerr
j ^common

^p11
=6DSPTIG41
=2V4.1
c %0\acad11\dsptig41.exp %7:%5 ^cerr
c %0\acad11\dsptig41.rlm c:\tiga ^cerr
e %8 2 ^p11g
e %8 3 ^p11f
c %0\acad11\dsptig41.uk %7:%5\DSPTIG41.CMD ^cerr
j ^common
^p11g
c %0\acad11\dsptig41.gr %7:%5\DSPTIG41.CMD ^cerr
j ^common
^p11f
c %0\acad11\dsptig41.fr %7:%5\DSPTIG41.CMD ^cerr
j ^common

^common
z
|Do you wish to make a sample batch file as C:\TIGA\%1.BAT ?
|
=3Y
@3Y/N: 
e %3 esc ^common
e "%3" "" ^common
e %3 n ^conclude
o C:\TIGA\%1.bat ^conclude
| Making...   C:\TIGA\%1.bat 
|
e %9 y ^protect
~TIGACD
~%7:
~CD %5
~ADICFG
~%6
~ACAD
~%6 -U
C
j ^conclude

^protect
~TIGACD
~%7:
~CD %5
~SET DSPADI=%7:%5\%6
~ACAD
C
j ^conclude

^conclude
z
|This concludes the installation of TIGA AutoCAD Release %4 Driver.
i %7:%5
e %9 y ^readme
|To run AutoCAD Rel.%4 with EIZO TIGA driver properly, follow as below.
|
|  1. Execute the TIGA graphics interface program (TIGACD.EXE) with the
|     video mode you wish.
|  2. Change to the AutoCAD Rel.%4 directory %7:%5.
|  3. Execute the driver configuration program (ADICFG.EXE) which
|     enables you to change some options available. And you may save new
|     configuration instead of default setting after setting new options.
|  4. Execute the ADI driver (%6.EXE) and ACAD program.
|  5. When you see the Main Menu, select '5. configure AutoCAD' to configure
|     new driver.
|  6. When at the configuration, select '3. Configure video display' and
|     select 'ADI display %2' from the list available, then follow the
|     instructions to complete the configuration.
j ^endreadme
^readme
|To run AutoCAD 386 (Rel.%4) with EIZO TIGA driver properly, follow as below.
|
|  1. Set the environment variable by typing the command 'SET DSPADI=
|     [d:][path]%6' at the DOS prompt, or add the command into your
|     AUTOEXEC.BAT file. AutoCAD 386 (Rel.%4) will search for the functional
|     driver file with this name automatically.
|  2. Execute the TIGA graphics interface program (TIGACD.EXE) with the
|     video mode you wish.
|  3. Change to the AutoCAD 386 (Rel.%4) directory %7:%5.
|  4. When you see the Main menu, select '5. configure AutoCAD' to configure
|     new driver.
|  5. When at the configuration, select '3. Configure video display' and
|     select 'ADI P386 %2 display' from the list available, then follow
|     the instructions to complete the configuration.
^endreadme
e %3 n ^finish
|
|Use the batch file C:\TIGA\%1.BAT created in order to run AutoCAD.
^finish
b
^cerr
z
|
|Error occurred. 
b
^tigaerr
z
|
|Unable to find EIZO TIGA Communications Driver (TIGACD.EXE) in the C:\TIGA.
|Please install TIGA system first.
b
