f c:\tiga\tigacd.exe ^tigaerr
T0 TIGA FastCAD Driver Installation
Di0
j ^wf

^hnotf
z
|Invalid target drive and directory specification
|
!Hit any key to return.
^wf
z
|Type the target drive to copy the FastCAD driver to.
|
=1C
@1Target Drive (C-Z): 
e %1 esc ^wf
e "%1" "" ^wf
z
|Type the target directory to copy the FastCAD driver to.
|
=2\FCAD
@2Target Directory : 
e %2 esc ^wf
=40
f %1:%2\fcad.exe ^hnotf
f %1:%2\dsdrv.bin ^nobin
f %1:%2\dsdrv.old ^noold
z
|You have a DSDRV.BIN file which you may want to save. AUTOINS normally
|saves this under the name DSDRV.OLD, but DSDRV.OLD already exists.
|AUTOINS will overwrite your DSDRV.BIN as DSDRV.OLD.
!Hit any key to continue
^noold
c %1:%2\dsdrv.bin %1:%2\dsdrv.old ^cerr
=41
^nobin
z
c %0\fcad\fcadsys.rlm c:\tiga ^cerr
c %0\fcad\dstiga.bin %1:%2\dsdrv.bin ^cerr
c %0\fcad\loadrlm.exe %1:%2 ^cerr
^common
z
|Do you wish to make a sample batch file as C:\TIGA\TIGAFCAD.BAT ?
|
=3Y
@3Y/N: 
e %3 esc ^common
e "%3" "" ^common
e %3 n ^conclude
o C:\TIGA\TIGAFCAD.BAT ^conclude
| Making...   C:\TIGA\TIGAFCAD.BAT 
|
~TIGACD
~%1:
~CD %2
~ADJUST DSDRV.BIN
~LOADRLM
~FCAD
~LOADRLM /U
C

^conclude
i %1:%2
z
|This concludes the installation of TIGA FastCAD Driver.
e %4 0 ^notsaved
|And your old video driver DSDRV.BIN was saved as the name DSDRV.OLD.
^notsaved
|To run FastCAD with EIZO TIGA driver properly, follow as below.
|
|  1. Execute the TIGA graphics interface program (TIGACD.EXE) with the
|     video mode you wish.
|  2. Change to the FastCAD directory %1:%2.
|  3. Execute the program LOADRLM to load the remote module and then
|     run FCAD program.
|  4. FastCAD automatically load the display driver DSDRV.BIN which is
|     copied and renamed from the file %1:\FCAD\DSTIGA.BIN.
e %3 n ^finish
|
|Use the batch file C:\TIGA\TIGAFCAD.BAT created in order to run FastCAD.

^finish
b
^cerr
z
|
|Error occurred. 
b
^tigaerr
z
|
|Unable to find EIZO TIGA Communications Driver (TIGACD.EXE) in the C:\TIGA.
|Please install TIGA system first.
b
