f c:\tiga\tigacd.exe ^tigaerr
T0 TIGA MicroStation PC Driver Installation
Di0
j ^wf

^hnotf
z
|Invalid target drive and directory specification
|
!Hit any key to return.
^wf
z
|Type the target drive to copy the MicroStation driver to.
|
=1C
@1Target Drive (C-Z): 
e %1 esc ^wf
e "%1" "" ^wf
z
|Type the target directory to copy the MicroStation driver to.
|
=2\USTATION
@2Target Directory : 
e %2 esc ^wf
f %1:%2\msmce.exe ^hnotf
z
c %0\mgl\mglsys.rlm c:\tiga ^cerr
c %0\mgl\bsivtiga.exe %1:%2\drivers ^cerr
c %0\mgl\bsivtiga.mgl %1:%2\drivers ^cerr
^conclude
i %1:%2
z
|This concludes the installation of TIGA MicroStation Driver.
|To run MicroStation with EIZO TIGA driver properly, follow as below.
|
|  1. Execute the TIGA graphics interface program (TIGACD.EXE) with the
|     video mode you wish.
|  2. Change to the MicroStation directory %1:%2.
|  3. Execute the configuration program USCONFIG, that is delivered as part
|     of the MicroStation software package, with proper responses as below.
|
|       a. Select "Modify Display Adapters" from Main Menu.
|       b. Select "Vendor Supplied Driver" for Primary Graphics Adapter.
|       c. Select "MGL:EIZO TIGA DRIVER" from the list available.
|       d. Select "No Second Adapter" or other video adapter you install.
|
|  4. After accomplishing USCONFIG, type MCE at the directory %1:%2.
|  5. Load the menu by typing the command "am=ustn,sb1" after drawing.
|
^finish
b
^cerr
z
|
|Error occurred. 
b
^tigaerr
z
|
|Unable to find EIZO TIGA Communications Driver (TIGACD.EXE) in the C:\TIGA.
|Please install TIGA system first.
b
