f c:\tiga\tigacd.exe ^tigaerr
T0 TIGA WordPerfect (Version 5.1) Driver Installation 
j ^top

^hnotf
z
|
|Invalid drive and directory specification
!Hit any key to return.

^top
z
|
|Type the drive and directory where WordPerfect has been installed.
=3C:\WP51
@3The drive and directory: 
e %3 esc ^hnotf
e "%3" "" ^top
f %3\install.exe ^hnotf
z
dis
z
|
|Installing...  TIGA WordPerfect Driver from %s
c %s\WP51\*.vrs %3 ^errend
c %s\WP51\*.rlm c:\tiga ^errend
^errok
z
|
|This concludes the installation of TIGA WordPerfect Driver.
|To run WordPerfect with EIZO TIGA driver properly, follow as below.
|
|  1. Execute the TIGA graphics interface program (TIGACD.EXE) with the
|     video mode you wish.
|  2. Run WordPerfect by typing "WP" and <Enter> at DOS prompt.
|  3. To select (Setup), press <Shift>+<F1> key.
|  4. To select (Display), press <2> or <D> key.
|  5. To select (Graphics Screen Type), press <2> or <G> key.
|  6. Move the pointer to the TIGA graphics driver and press <Enter> key.
|  7. Reply for Duplex screen / Graphics.
|  8. To select (Text Screen Type), press <3> or <T> key.
|  9. Move the pointer to the TIGA text driver and press <Enter> key.
| 10. Reply for Duplex screen or Full screen / Graphics.
|
|Refer to the TIGA Installation Manual for detail.
|
b
^errend
|
|Error occurred.
|Please reinstall.
b
^tigaerr
z
|
|Unable to find EIZO TIGA Communications Driver (TIGACD.EXE) in the C:\TIGA.
|Please install TIGA system first.
b
