f c:\tiga\tigacd.exe ^tigaerr
Dis
^loop1
z
T0TIGA Ventura & GEM Driver Installation
| Select the item you wish to install and press Enter, or type the number.
|
S1 Ventura Publisher V2.0/V3.0 Installation
S2 GEM/3 Release 3.01/3.1 Installation          
S3 Quit this Installation Program          
W0 
e %0 1 ^vp
e %0 2 ^gem
e %0 3 ^end
e %0 esc ^end
j ^loop1

^vpnf
z
|
|Invalid drive specification
!Hit any key to return.

^vp
z
T0TIGA Ventura Publisher Driver Installation
|
|Ventura Publisher V2.0/V3.0 needs to be installed using VGA graphics
|as display adapter before running this AUTOINS program.
|
|Which drive is the Ventura Publisher V2.0/V3.0 installed?
=1C
@1Drive (C-Z): 
e %1 esc ^loop1
f %1:\VENTURA\DRVRMRGR.EXE ^vpnf
f %1:\VP.BAT ^novpbat
=6 VP.BAT
j ^screen
^novpbat
f %1:\VPPROF.BAT ^vpnf
=6 VPPROF.BAT

^screen
^sloop
z
|
|You can use TIGA Ventura Driver with Large System Font if you prefer.
|But it cannot be used with 8 bit/pixel mode.
|
|Do you wish to use Large System Font?
=5N
@5Y/N: 
e %5 esc ^vp
e y %5 ^dtigalf

=5 SDTIGA.VGA
j ^install

^dtigalf
=5 SDTIGALF.VGA

^install
z
|
|Installing...  TIGA Ventura Publisher Driver from %s
|
c %s\%5 %1:\VENTURA ^errend
c %s\textout.rlm c:\tiga ^errend
^makebat
z
|
|The batch file %1:\%6 is found. In order to run Ventura under TIGA
|properly, AUTOINS needs to modify your %1:\%6 or to make another
|batch file.
|
|Do you wish to modify your %1:\%6 to run Ventura under TIGA?
=2Y
@2Y/N: 
z
e %2 y ^autochange
e %2 esc ^makebat
|
|Do you wish to make a sample batch file as C:\TIGA\TIGAVP.BAT ?
=2Y
@2Y/N: 
z
e %2 y ^maketoc
e %2 esc ^makebat
|
|This concludes the installation of TIGA Ventura Publisher Driver.
|
|Refer to TIGA Installation Manual to run Ventura under TIGA.
j ^virtual

^maketoc
c %1:\%6 C:\TIGA\TIGAVP.BAT ^errend
=1C
=6 TIGA\TIGAVP.BAT
^autochange
#%s\modtext %1:\%6 TIGACD @
#%s\modtext %1:\%6 %5_ DRVRMRGR /S= /M
i %1:\
z
|
|This concludes the installation of TIGA Ventura Publisher Driver.
|
|Use %1:\%6 in order to run Ventura Publisher under TIGA.
^virtual
|
|TIGA Ventura Publisher Driver provides you VIRTUAL SCREEN which extends
|the drawing area out of screen and enables you to see the whole drawing
|area by scrolling with mouse cursor. If you wish to see VIRTUAL SCREEN
|with Ventura, turn <Scroll Lock> key OFF before you start Ventura.
|Otherwise turn <Scroll Lock> key ON.
b


^gemnf
z
|
|Invalid drive specification
!Hit any key to return.

^gem
z
T0TIGA GEM/3 Release 3.01/3.1 Driver Installation
T1 
|
|GEM/3 Release 3.01/3.1 needs to be installed using VGA graphics
|as display adapter before running this AUTOINS program.
|
|Which drive is the GEM/3 installed?
=1C
@1Drive (C-Z): 
e %1 esc ^loop1
f %1:\GEMAPPS\GEMSYS\GEMVDI.EXE ^gemnf
=5 SDTIGAG3.VGA

^mouse
z
|Which mouse do you have? 
^mgemloop
SA No Mouse                                          
SB Bus Mouse (Requires file MOUSE.COM)               
SC IBM Personal System/2 Mouse                       
SD Microsoft Serial Mouse (RS232)                    
SE Mouse Systems PC Mouse / SummaMouse / Compatibles 
W6Please select the mouse you have, and press Enter key.  [PgUp] : next page
e %6 esc ^gem
e a %6 ^nomouse
e b %6 ^atmouse
e c %6 ^psmouse
e d %6 ^msmouse
e e %6 ^pcmouse
e pageup %6 ^mgemloop2
j ^mgemloop

^mgemloop2
SF SummaSketch 961 Cursor-Type Tablet                
SG SummaSketch 961 Stylus-Type Tablet                
SH SummaSketch 1201 Cursor-Type Tablet               
SI SummaSketch 1201 Stylus-Type Tablet               
SJ Summagraphics MM1812 Cursor-Type Tablet           
SK Summagraphics MM1812 Stylus-Type Tablet           
W6Please select the mouse you have, and press Enter key.  [PgDn] : prev. page
e %6 esc ^gem
e f %6 ^sm961cu
e g %6 ^sm961st
e h %6 ^sm1201cu
e i %6 ^sm1201st
e j %6 ^sm1812cu
e k %6 ^sm1812st
e pagedown %6 ^mgemloop
j ^mgemloop2

^nomouse
=6 0
=7 3
j ^gemcopy

^pcmouse
=6 1
j ^comm

^atmouse
=6 2
=7 3
j ^gemcopy

^msmouse
=6 3
j ^comm

^psmouse
=6 :
=7 3
j ^gemcopy

^sm1201st
=6 4
j ^comm

^sm1201cu
=6 5
j ^comm

^sm961st
=6 6
j ^comm

^sm961cu
=6 7
j ^comm

^sm1812st
=6 8
j ^comm

^sm1812cu
=6 9
j ^comm

^comm
z
|Which communication port are you using for the mouse? 
SA Communication Port #1 
SB Communication Port #2 
W7Please select the communication port you are using, and press Enter key.
e %7 esc ^mouse
e b %7 ^commb
n a %7 ^comm

^comma
=7 0
j ^gemcopy

^commb
=7 1
j^gemcopy

^gemcopy
z
|
| Installing ...  TIGA GEM/3 Driver
|
d %1:\gemapps\gemsys\sd*.vga ^gemnf
c %s\%5 %1:\gemapps\gemsys ^errend
c %s\textout.rlm c:\tiga ^errend
e 3 %7 ^noport
e 0 %7 ^port1
=7 4
j ^chkmt
^port1
=7 3
j ^chkmt
^noport
=7 255
^chkmt
n : %6 ^setmp
=6 10
^setmp
#%s\setmp %1:\gemapps\gemsys\%5 %7 %6
i %1:\
z
|
|This concludes the installation of TIGA GEM/3 Driver.
|
|Run %1:\GEM.BAT at DOS prompt.
b
^tigaerr
z
|
|Unable to find EIZO TIGA Communications Driver (TIGACD.EXE) in the C:\TIGA.
|Please install TIGA system first.
b
^errend
|
|Error occurred.
|Please reinstall.
b
