InS_StArT
IBMENIO.COM
1.0
^IBMENIO,IBMENIO.COM,IE0
?Please select the options that match your board's settings.
!RIE0(INT)Hardware Interrupt
2
@3
4
5
7
9
10
11
!RIE0(PORT)Base I/O Port
240
280
2C0
@300
320
340
360
!RIE0(MEM) Base Memory Address
C8000
CC000
@D0000
D4000
D8000
DC000
!RIE0(ADAPTER ACCESS)Adapter access type
?The adapter access type must match the hardware configuration.
@I/O
RAM
$OIE0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*RIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
