InS_StArT
MPCO.COM
1.0 
^Auto Busmaster MC 32 Adapter,MPCO.COM,00M
^Auto Busmaster PCI Adapter,MPCO.COM,000
!O00M()Slot
?For microchannel adapters only, select the slot number that corresponds to the expansion slot where the adapter is installed.  Ignore this parameter for PCI adapters; use the PCISLOT parameter instead.
SLOT 1
SLOT 2
SLOT 3
SLOT 4
SLOT 5
SLOT 6
SLOT 7
SLOT 8
!O000()PCI Slot
?For PCI adapters only, select the slot number that corresponds to the expansion slot where the adapter is installed.  Ignore this parameter for Microchannel adapters; use the SLOT parameter instead.
PCISLOT 17
PCISLOT 18
PCISLOT 19
PCISLOT 20
PCISLOT 21
PCISLOT 22
PCISLOT 23
PCISLOT 24
!O000()Datarate
?For PCI adapters only, select the datarate at which you want to send data, in Mbps, on the LAN.  A choice of AUTO means that the adapter will sense the datarate being used by the LAN, and set the adapter at that speed.
DATARATE 4
DATARATE 16
@DATARATE AUTO
$O00M(NODE ADDRESS)Optional Node Address
400000000000M
7FFFFFFFFFFFM
*RIEM(FRAME)Frame Type
@TOKEN-RING MSB 
TOKEN-RING_SNAP MSB
TOKEN-RING LSB
TOKEN-RING_SNAP LSB
!R00M(RXBUFFERS)Receive Buffers
?Enter the desired number of receive buffers:
1
@2
4
8
!R00M(TXBUFFERS)Transmit Buffers
?Enter the desired number of transmit buffers:
1
@2
4
!O00M()Dedicated Transmit Buffers
?If you are using Windows, EMM386.EXE, or other memory manager, please select this option.
USEDEDICATEDTXBUFS
InS_EnD
