InS_StArT
ET32ODI.COM
1.0
^KTI ET32/P2 PCI Ethernet Adapter,ET32ODI.COM,000
^KTI ET32/PC PCI Ethernet Adapter,ET32ODI.COM,000
^KTI ET32/PT PCI Ethernet Adapter,ET32ODI.COM,000
$OIE0 (NODE ADDRESS) 10- Node Address
0
7FFFFFFFFFFF
*OIE0 (FRAME) 01- Media Frame Type(s)
?Note: Ethernet_802.2 is the default frame type for many NetWare servers.  Newer servers default to Ethernet_802.2 frame type.  Check with your administrator for the correct frame type for your network.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!OIE0 (PCIBOARD) 02- PCI Board Number
?Note: This parameter is used to specify a adapter when multiple adapters are used.  (none) - auto scan by driver
1
2
3
4
InS_EnD
