InS_StArT
SMCPWR.COM
1.0
^Standard Microsystems Corporation 8432/8434/9332 PCI,SMCPWR.COM,0E0
?This driver supports PCI machines
$O0E0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*O0E0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!O0E0()Media Access Type
?NOTE: Media access type will be autodetected on driver's load
TP
TP_NO_LINK_TEST
TP_FULL_DUPLEX
AUI
BNC
@AUTOSENSE 
!O0E0(Line_Speed)Line Speed
?NOTE: The default Line speed will be selected on driver's load according to the chip found in board (Ethernet or Fast-Ethernet).
10
100
InS_EnD




 
