InS_StArT
3C79x.COM
1.1
^3Com 3C79x FDDILink PCI (3C79x),3C79x.COM,0000P0
?The 3Com 3C79x FDDILink PCI DOS ODI Client Driver is the terminate-stay-resident (TSR) device driver for the DOS environment.	This driver works with the 3Com 3C79x FDDILink PCI Fiber or UTP adapter.
$O0000P0(PCICARD)PCI Card Number ( default = 1 )
?Enter the PCI card (instance) number of the 3Com 3C79x FDDILink PCI for this bus number.
1
4
@1
$O0000P0(MAX FRAME SIZE)Max Frame Size ( default = 4491 )
?Enter the maximum frame size for this adapter.  Normally the driver advertises the maximum frame size allowed for FDDI (4491 bytes) but this parameter may be used to lower the setting.
16
4491
@4491
$O0000P0(TREQ)Requested TTRT  ( default = 8 )
?Enter the desired MACTReq value in milliseconds.  Normally this parameter does not need to be changed from the default value of 8 ms.
4
165
@8
!O0000P0(FULLDUPLEX)Full-Duplex Mode ( default = OFF )
?Enter whether FDDI Full-Duplex (FDX) mode should be enabled on the adapter.
@OFF
ON
*R0000P0(FRAME)Media Frame Type(s)
@FDDI_802.2
FDDI_SNAP
InS_EnD
