InS_StArT
AT24ODI.COM
1.0
^ATI Ethernet AT2450,AT24ODI.COM,IE0
?This is the DOS ODI driver for the AT2450T, AT2450BT, AT2450FT and AT2450AT.
$OIE0(NODE ADDRESS)Optional Node Address
0
7FFFFFFFFFFF
*RIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
