InS_StArT
CPQNF3.COM
1.0
^Compaq Netelligent/NetFlex-3 Controller,CPQNF3.COM,0E0
?This driver supports the Compaq Netelligent/NetFlex-3 controllers.
$O0E0 (SLOT) EISA/PCI Slot Number
?This parameter is only necessary if you have multiple Compaq NetFlex-3 controllers in your system.  If not specified the first controller found will be used.
0
255
$O0E0 (NODE ADDRESS) Node Address
0
7FFFFFFFFFFF
*O0E0 (FRAME) Media Frame Type(s)
Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!O0E0 () UTP Media Connector
?Specify this parameter to use ONLY the RJ45 connector.  This is needed if you are connected to a hub that does not provide link signal.  Autosense is enabled in the absence of this parameter.
UTP
!O0E0 () AUI Media Connector
?Specify this parameter to use ONLY the AUI connector.  This is needed if you are connected to a hub that does not provide link signal.  Autosense is enabled in the absence of this parameter.
AUI
!O0E0 () Force 10mbit/sec Full Duplex Mode
?This parameter will force 10mbit/sec Full Duplex mode.  Specify this parameter ONLY if your controller is connected to a Full Duplex hub.  Half Duplex is the default mode.
10FD
!O0E0 () Force 100mbit/sec Full Duplex Mode
?This parameter will force 100mbit/sec Full DUplex mode.  Specify this parameter ONLY if your controller is connected to a Full Duplex hub.  Half Duplex is the default mode.
100FD
InS_EnD

