InS_StArT
CPQTRPCI.COM
1.1
^Compaq Netelligent 4/16 TR PCI UTP/STP Controller,CPQTRPCI.COM,0000P0
!O0000P0(SPEED) Line Speed (in Mbps)
?Select none to follow the adapter's default setting.  If you wish to override the default setting, make another selection.
4
16
$O0000P0(MAX FRAME SIZE) Maximum Frame Size
?Select Maximum Frame Size; default is 4216. Larger frame sizes may improve performance. MAX FRAME SIZE above 4216 is allowed only if Speed is 16 Mbps. 
632
17960
!O0000P0() Disable Early Token Release
?Select DETR to disable Early Token Release for 16Mbps networks.
DETR
!O0000P0() Reinsert
?In most cases, select none.  If you want the driver to reinsert into the ring after a MAC Remove Frame is received, select Reinsert.
REINSERT
*R0000P0(FRAME) Frame Type
?The driver defaults to the TOKEN-RING frame type.  TOKEN-RING_SNAP is also available.
@TOKEN-RING MSB
TOKEN-RING_SNAP MSB
$O0000P0(NODE ADDRESS) Node address
?Select none unless you want to set a locally administered Node ID in the range shown.
400000000000
40007FFFFFFF
InS_EnD
