InS_StArT
DC21X4.COM
1.0
^Digital Semiconductor 2104x/2114x 10/100 mbps Ethernet Controller,DC21X4.COM,0E0
?This driver supports Digital Semiconductor 2104x/2114x 10/100 mbps Ethernet Controller based Network adapters on PCI machines.
$O0E0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*O0E0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!O0E0()Connection Type
?NOTE: Connection type will be autodetected on driver's load
TP
TP_NO_LINK_TEST
TP_FULL_DUPLEX
AUI
BNC
T4
@AUTOSENSE 
!O0E0(Line_Speed)Line Speed
?NOTE: The default Line speed will be selected on driver's load according to the chip found in board (Ethernet or Fast-Ethernet).
10
100
!O0E0()Power Saving Mode
?NOTE: Select the SNOOZE mode if you wish the chip to work in Power-Saving mode.
SNOOZE
InS_EnD




 
