InS_StArT
DE425.COM
1.0
^DEC EtherWORKS TURBO EISA (DE425),DE425.COM,0E0,DEC4250
?Digital EtherWORKS Turbo EISA DOS ODI Client Driver is the terminate-stay-resident (TSR) device driver for the DOS environment. 
$O0E0(SLOT)Slot Number                   
1
15
$O0E0(NODE ADDRESS)Node Address
0
FFFFFFFFFFFF
*R0E0(FRAME)Media Frame Type(s)                                 
@ETHERNET_802.2
ETHERNET_II
ETHERNET_SNAP
ETHERNET_802.3
InS_EnD


