InS_StArT
DE660.COM
1.0
^D-Link DE-660 Family,DE660.COM,IE0
?Please select the options that match your board's IO settings.
!RIE0(PORT)
@300
320
340
360
200
220
240
260
$OIE0(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*RIE0(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
