InS_StArT
DIVAPCM.BAT
1.0,DIVAPRE.EXE,TED5ESS.EXE,TEDATEL.EXE,TEDJAPAN.EXE,TEDNI.EXE,TED1TR6.EXE,TEDBELG.EXE,TEDETSI.EXE,TEDFRANC.EXE,TEDSWED.EXE,DPMS.EXE,V110.BIN,KERNEL05.BIN,HSCX.BIN,FAX.BIN,AFAX2.EXE,ACOPY2.EXE,ACOPY.EXE,DIDD.386,DIMAINT.EXE,DILOG.EXE,DIINFO.EXE,DIMAINT.386,CAPI20.DLL,CAPI.DLL,DIAPIS.EXE,CAPI20.EXE,VCAPID.386,API_MAP.EXE,DIVAPCM.EXE
^Diva Classic PC-Card,DIVAPCM.BAT,IE0000
)CAPIISDN
?Please select an available I/O port.
!RIE0000(PORT)
200
220
@240
260
280
2A0
2C0
2E0
300
320
340
360
380
3A0
3C0
3E0
!RIE0000(IRQ)
2
3
4
@10
11
12
!RIE0000(D-CHANNEL PROTOCOL)D-Channel Protocol
?Please select your country.
AT&T 5ESS Custom (w/SPIDs for Multi-Point)
Australian national ISDN protocol
Belgian national ISDN protocol
Euro ISDN E-DSS1
French national ISDN protocol
German national ISDN protocol 1TR-6
ITU Q.931
Japanese national ISDN protocol
@National ISDN 1 and NT DMS100 (w/SPIDs)
Nortel Custom (w/SPIDs for Multi-Point)
Swedish national ISDN protocol
!RIE0000(TRACE)TRACE
?Enable ISDN traces.
Yes
@No
!RIE0000(DIRECT)DIRECT_enabler
?Use direct PCMCIA enabler (no card and socket services)
@No
Yes
InS_EnD

