InS_StArT
E10PODI.COM
1.0
^Intel EtherExpress(TM) PRO/10 PCI LAN Adapter,E10PODI.COM,IE0
?This is the DOS ODI driver for the Intel EtherExpress(TM) PRO/10 PCI LAN adapter.
$O000(PCISLOT) Optional PCI Slot Num
?This DOSODI driver supports 15 PCI slots.  A PCI slot signifies the Device ID shifted by 3 to mask off the function number. This parameter is optional.
1
15
$O000(FIFO) Optional FIFO Threshold
?Specify the FIFO threshold value to be used by the 82596 LAN controller.
1
15
$O000(ON) Optional T-ON Value
?Specify the T-ON Bus Throttle value for the 82596 LAN controller.
0
64535
$O000(OFF) Optional T-OFF Value
?Specify the T-OFF Bus Throttle value for the 82596 LAN controller.
0
64535
*O0E0(FRAME) Frame Type
?Note: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
$O0E0(NODE ADDRESS) Adapter Node Address
?Warning: Entering an incorrect value for the node address can cause serious network problems. If you are uncertain, leave the node address blank.
0
FFFFFFFFFFFF
InS_EnD
