InS_StArT
HPFEODIM.COM
1.1
^Hewlett-Packard DeskDirect 10/100 Bus Master LAN Adapter,HPFEODIM.COM,IE0
?Note: The driver is self-configuring, which means no NET.CFG parameters are needed. Only one PORT, SLOT, BUS ID, or CARD ID may be specified.
$OIE00P0 (PORT) Optional Base I/O Port
?Note: For ISA cards, this parameter must be between 100 and 3C0 on the 40 boundary. For PCI cards, this parameter must be between C000 and FF00 on the 100 boundary. This parameter is not valid for EISA cards. All numbers are hexadecimal here.
100
FF00
$O0E00P0 (SLOT) Optional EISA/PCI Slot
?Note: This parameter is only valid for the EISA and PCI adapters. For EISA cards, it's between 1 and 15. For PCI adapters, it is only valid when the adapter is installed on the PC's with PCI BIOS ver 2.10 or later and must be between 1 and 255.
1
255
!OIE0 (BUS ID) Optional Bus Identifier
ISA 0
EISA 2
PCI 4
$OIE0 (CARD ID) Optional Card Identifier
?Note: The last six hex digits of the cards MAC address.
0
FFFFFF
!OIE0 (INT) Optional Hardware Interrupt
?Note: This parameter is not valid for the PCI adapter.
3
4
5
7
9
10
11
12
15
*OIE0 (FRAME) Optional Media Frame Type(s)
?Note: Ethernet_802.2 is now the default frame type for ODI drivers.  Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
!OIE0 (LAN SPEED) Optional LAN Speed
?Note: Force the adapter to use only the specified port.
10
100
$OIE0 (NODE ADDRESS) Optional Node Address
0
7FFFFFFFFFFF
InS_EnD
