InS_StArT
IBMEANWC.COM
1.0
^IBM PCI Ethernet Adapter,IBMEANWC.COM,IE0
?This driver supports the IBM PCI Ethernet Adapter.
!RIE0(BusType)Bus Type
?Specify the method used to search the PCI bus.
PCI1
@PCI2
!OIE0(FDUP)Full Duplex
?Full Duplex may be specified for either the UTP or AUI connection, or turned off (default).
UTP
AUI
OFF
!OIE0(LED0)Function of Green LED near AUI connector
?Optionally program the Green LED: 81 = Network collisions, 84 = Network activity, 82 = Jabbering, 90 = Transmitting, A0 = Receiving, B0 = Transmitting/receiving, C0 = Link status (default), 88 = Receive polarity, 180 = Full duplex.
81
84
82
90
A0
B0
C0
88
180
!OIE0(LED1)Function of Amber LED near AUI connector
?Optionally program the Amber LED: 81 = Network collisions, 84 = Network activity, 82 = Jabbering, 90 = Transmitting, A0 = Receiving, B0 = Transmitting/receiving (default), C0 = Link status, 88 = Receive polarity, 180 = Full duplex.
81
84
82
90
A0
B0
C0
88
180
!OIE0(LED2)Function of Green LED near RJ45 connector
?Optionally program the Green LED: 81 = Network collisions, 84 = Network activity, 82 = Jabbering, 90 = Transmitting, A0 = Receiving, B0 = Transmitting/receiving, C0 = Link status, 88 = Receive polarity, 180 = Full duplex (default).
81
84
82
90
A0
B0
C0
88
180
$OIE0(NODE ADDRESS)Node Address
0
7FFFFFFFFFFF
*RIE0(FRAME)Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
