InS_StArT
IBMEXNWC.COM
1.0
^IBM EtherJet PC Card,IBMEXNWC.COM,IEM
!OIEM(ENABLE)PC Card Environment (optional)
?Specify PCMCIA or (none) to use full PCMCIA support in IBMEXNWC.COM.  Specify NOPCMCIA if using POINTJET.EXE or CS20JET.EXE to enable the PC Card.  If the ENABLE parameter is not present, IBMEXNWC.COM uses only card services to locate the PC Card.
PCMCIA
NOPCMCIA
!OIEM(INT)Hardware Interrupt (optional)
3
4
5
6
7
9
10
11
12
14
15
!OIEM(PORT)Base I/O Port (optional)
200
210
220
230
240
250
260
270
280
290
300
310
320
330
340
350
360
!OIEM(SLOT)Slot (optional)
?For this adapter, the slot keyword specifies the socket of the PC Card.  This parameter is ignored if ENABLE NOPCMCIA is specified.
1
2
3
4
5
6
7
8
!OIEM(DUPLEXMODE)Duplex Mode (optional)
?Specify HDX or (none) for forced half duplex operation.  Specify FDX for forced full duplex operation.  Specify AUTO to allow autonegotiation.
HDX
FDX
AUTO
$OIEM(NODE ADDRESS)Node Address (optional)
0
FFFFFFFFFFFF
*OIEM(FRAME)Media Frame Type(s) (optional)
?NOTE:	Ethernet_802.2 is the default frame type for ODI Drivers.  Existing LANs may be using Ethernet_802.3.
Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD
