InS_StArT
MCBODI.COM
1.0
^Madge 16/4 CardBus Token-Ring Adapter,MCBODI.COM,IE0
?If your network is using Source Routing please load ROUTE.COM after MCBODI.COM. This adapter requires a Card Services interface to be present. This can be provided using the Madge Card Services Emulator (MADGECS.EXE) or by third party software. To allow hot-swapping of this adapter add the keyword "HOTSWAP" to the "LINK DRIVER MCBODI" section of NET.CFG
$OIEM(PORT) Base I/O Port
?Enter the Base I/O Location of the Ringnode to be used. This parameter is not required if there is just a single Madge CardBus Adapter in your machine.
0000
FFFF
$OIEM(SLOT) CardBus Slot number
?Enter the CardBus slot location of the Ringnode to be used. This parameter is not required if there is just a single Madge CardBus Adapter in your machine.
0
FFFF
!OIEM(FRAME) Frame Type
TOKEN-RING MSB
TOKEN-RING LSB
TOKEN-RING_SNAP MSB
TOKEN-RING_SNAP LSB
$OIEM(NODE ADDRESS) Node Address
400000000000
7FFFFFFFFFFF
!OIEM() Hot-swapping Support
?Select HOTSWAP if you require the ability to remove and replace your CardBus adapter without unloading and reloading the driver and protocol stack. Note, that before the card is removed you should log out of any network resources.
HOTSWAP
!OIEM(MAX FRAME SIZE) Maximum frame size
?Select the maximum packet size for your network. Default is 4210.
626
1138
2162
4210
8000
18000
InS_EnD
