InS_StArT
NE2000.COM
1.1
^Novell Ethernet NE2000,NE2000.COM,IE0000
^Eagle NE2000,NE2000.COM,IE0000
^Eagle NE2000PLUS,NE2000.COM,IE0000
^Eagle NE2000PLUS 3,NE2000.COM,IE0000
^Eagle NE2000PLUS T,NE2000.COM,IE0000
^Microdyne NE2000,NE2000.COM,IE0000
^Microdyne NE2000PLUS,NE2000.COM,IE0000
^Microdyne NE2000PLUS T,NE2000.COM,IE0000
^Microdyne NE2000PLUS 3,NE2000.COM,IE0000
^National Semiconductor NE2000 InfoMover,NE2000.COM,IE0000
^ATI AT-2000T Plus,NE2000.COM,IE0000
^ATI AT-2000U Plus,NE2000.COM,IE0000
?Please select the options that match your board's jumper settings.
!RIE0000(IRQ)
2
@3
4
5
10
11
12
15
!RIE0000(PORT)
@300
320
340
360
240
280
2C0
!OIE0000(MEM)
D0000
D4000
D8000
DC000
C0000
C4000
C8000
CC000
$OIE0000(NODE ADDRESS)Optional Node Address
0
FFFFFFFFFFFF
*RIE0000(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
InS_EnD

VeRsIoN=2.00  Novell NE2000 Ethernet MLID installation file.
CoPyRiGhT=(c) Copyright 1993 - 1996, by Novell, Inc. All rights reserved.

