InS_StArT
TCVG45.COM
1.0
^Thomas-Conrad VG45 ISA Adapter,TCVG45.COM,I00
?Please select the options for your adapter.
!OI00(PORT) Base I/O Address
?If none is selected, the driver will scan the I/O ports for an adapter.
100
140
180
1C0
200
240
280
2C0
@300
340
380
*OIE0(FRAME) Frame Type
?The driver defaults to the ETHERNET_802.2 frame type.
ETHERNET_802.2
ETHERNET_802.3
ETHERNET_II
ETHERNET_SNAP
$OIE0(NODE ADDRESS) Node Address override
?This option allows you to specify a node address in the range shown below.
008013000000
008013FFFFFF
InS_EnD
