InS_StArT
TCVG47.COM
1.0
^Thomas-Conrad VG47 EISA Adapter,TCVG47.COM,0E0
?Please select the options for your adapter.
!O0E0(SLOT) Slot
?If none is selected, the driver will scan the EISA bus for an adapter.
1
2
3
4
5
6
7
8
9
10
11
12
13
14
15
*OIE0(FRAME) Frame Type
?The driver defaults to the ETHERNET_802.2 frame type.
ETHERNET_802.2
ETHERNET_802.3
ETHERNET_II
ETHERNET_SNAP
$OIE0(NODE ADDRESS) Node Address override
?This option allows you to specify a node address in the range shown below.
008013000000
008013FFFFFF
InS_EnD
