InS_StArT
WVLAN05.COM
1.0
^WaveLAN,WVLAN05.COM,IEMA00,6A14
?This driver is intended for a WaveLAN NIC. WaveLAN NICs are available for ISA (AT bus), microchannel bus or PCMCIA type II slot. In case of ISA, the card must be in a 16-bits slot. If your machine is equipped with [E]ISA/MCA slots as well as a PCMCIA socket, you can use both type of WaveLAN NICs simultanuous. You can have a maximum of four WaveLAN network boards in your machine. Refer to your technical publications for directions how to select in that situation a particular card.
!0000A00(SOCKET)PCMCIA Socket
?If you are using a WaveLAN NIC in a PCMCIA socket, you may select the first available (X) or a particular PCMCIA socket (A-H).
A
B
C
D
E
F
G
H 
X
!0IE0000(PORT)Base I/O Port
?If you are using a WaveLAN NIC in an [E]ISA slot, you must select the option that matches your board's I/O jumper setting. The 3C0 setting may conflict with EGA video cards. The 3E0 setting may conflict with COM3.
300
390
3C0
3E0
!000M000(SLOT)Slot location
?If 0 is selected, the driver scans for the WaveLAN network boards. It starts at slot 1 and uses the first WaveLAN board found.
0
1
2
3
4
5
6
7
8
*RIEMA00(FRAME)Media Frame Type(s)
?NOTE: Ethernet_802.2 is now the default frame type for ODI Drivers. Existing LANs may be using Ethernet_802.3.
@Ethernet_802.2
Ethernet_802.3
Ethernet_II
Ethernet_SNAP
$0IEMA00(NWID)WaveLAN Network ID
?This parameter defines the WaveLAN Network ID of the WaveLAN cell in which communication is required. It can also be defined with the INSTCONF/SETCONF utilities. If this parameter is not specified, it defaults to 0100.
0100
FFFF
@0100
$0IEMA00(DOMAIN ID)Domain ID
?This parameter must be used if the unit is used in a roaming environment. The Domain ID must match the value installed at the Access Points.
0000
FFFF
@0001
$0IEMA00(BEACON KEY)Beacon Key
?This parameter can be used if the unit is used in a roaming environment. The Beacon Key must match the value installed at the Access Points.
0000
FFFF
$0IEMA00(ENCRYPTION KEY)Encryption Key
?This parameter is required if encryption is used in the network. It may be defined here or with the INSTCONF/SETCONF utilities. The value must be identical in all systems of the network.
0000000000000000
FFFFFFFFFFFFFFFF
@0
$0000A00(Config Address)Config Address
?This parameter is used by the CS&SS Client Driver. It will be inserted in the NET.CFG by the WaveLAN CS&SS Install program.
000000000000
FFFFFFFFFFFF
$0000A00(POWER UP)Power Up time
?This parameter defines the time in seconds that the station will listen to server watchdog messages to keep the session alive. Unless the server parameters are changed, it is advised to use the default of 120 seconds.
0
65535
$0000A00(POWER DOWN)Power Down time
?This parameter defines the time in seconds that the station will be turned off if no traffic is expected. Unless the server parameters are changed, it is advised to use the default of 480 seconds.
0
65535
InS_EnD